What keys must be pressed during post on the PowerEdge M600 or M605 server module as the SAS 6 i/R is recognized, to enter the configuration utility?

   Ctrl and M  
 Ctrl and A  
 Ctrl and R  
== Ctrl and C 



When connected to the PowerEdge M1000e CMC through HyperTerminal, type connect switch-1 and press to connect to switch module 1.

  **** True  
 False 
=============================

The integrated SAS 6 i/R in the PowerEdge M605 supports Raid 5.

 ***  False 
 True 
==============================
The PowerEdge M600 and M605 hard-disk drives are hot swappable when using a SAS repeater daughter card.

  *** False 
 True 
=========================================
A null-modem cable can be used to connect between the CMC and the client system for configuration of the PowerEdge M1000e CMC.

   False 
 **** True 
====================================
The midplane on the PowerEdge M1000e is hot swappable.

   True 
 **** False  

============================
What physical component must be installed for the TCP Offloading Engine (TOE) to function on the PowerEdge M605 and M600 server modules?

   Second processor 
 Second NIC 
 NIC daughter card 
 *** TOE Key ?
===========================================
What is the default username and password for the CMC on the PowerEdge M1000e?

   calvin, hobbs 
 *** root, calvin ?
 admin, password 
 administrator, password 

==========================================
What keys must be pressed during post on the PowerEdge M600 or M605 server module as the SAS 6 i/R is recognized, 
to enter the configuration utility?

   Ctrl and R  
 Ctrl and A  
 Ctrl and M  
 *** Ctrl and C ?

===========================================
On the PowerEdge M600 or M605 server modules, what key must be pressed during POST to access the system setup?

   Esc 
 *** F2 ?
 F12 
 F8 
==============================================
Which internal storage controllers are supported in the PowerEdge M600 and M605.

  *** SAS 6/iR  ?
 SAS repeater daughter card  
 PERC 5/E 
 PERC 5/i 
========================================
Which type of hard disk drives are supported on the PowerEdge M600 and M605 server modules?

   3.5 inch SAS, 2.5 inch SAS and 3.5 inch SATA 
 3.5 inch SAS 2.5 inch SATA and 3.5 inch SATA 
 *** 2.5 inch SAS or 2.5 inch SATA ?
 3.5 inch SAS and 3.5 inch SATA 
===========================================
The asset tag utility should be used to set the service tag on a PowerEdge M600 or M605 blade service tag when:

  **** Replacing the system board ?
 A BIOS flash fails 
 Replacing the processors 
 Replacing both hard-disk drives 
==========================================
Which network card is integrated on the PowerEdge M600 and M605 server modules?

   Intel 82450 
 Broadcom BCM5704 
 *** Broadcom BCM5708 ?
 Intel 83451E1 
==========================================

How many USB ports are on the front of the PowerEdge M600 and M605 server modules?

   One 
 None 
 Four 
 *** Two ?
==========================================

When connected to the PowerEdge M1000e CMC through HyperTerminal, what command is used to view the network configuration of the CMC?

   racadm autonetwork  
 *** racadm getniccfg  
 racadm networkcfg  
 racadm setniccfg 
=======================================
How many hard-disk drives are supported in the PowerEdge M600 and M605 when using the SAS 6 i/R storage controller?

   Three 
 None 
 One 
 *** Two 
=====================================

The PowerEdge M1000e Ethernet passthrough module support what speed(s)?

   10/100 Mbps 
 100 Mbps 
 10 Mbps 
 *** 10/100/1000 Mbps  

 
=======================================
A customer reports that he has lost his iDRAC password and does not want to install OMSA, 
how can this password be recovered?

   The customer must replace the system board; this password is not recoverable. 
 The customer must re-flash the system BIOS to recover the password.  
 **** The customer can boot to the CTRL-E option and reset the iDRAC to default.  
 The customer must boot to the ASSET utility to replace this password.  

 
========================================
What command is used to copy the running configuration to the startup configuration on the PowerConnet 6220 switch module in the PowerEdge M1000e?

   move running-config startup-config 
 copy running-configurations startup-configurations 
 **** copy running-config startup-config 
 copy config startup-config 
=============================================

You have just changed from SAS to RAID using the SAS 6 i/R on a customers PowerEdge M605 server module. After performing this function you now see a post screen that reads 'F1 to continue or F2 to enter setup'. What must be done to configure this RAID functionality?

 A rebuild must occur before the OS will boot correctly. 
 *** Performing this action is destructive to data and the OS must be reinstalled. 
 The BIOS must be upgraded to support RAID functionality. 
 Inform the customer that the board seems to be faulty, call Dell to have it replaced. 
===========================================
The iDRAC in the PowerEdge M1000e allows what type of console redirection?

 Text-based only when using Hyper-Terminal.  
 Text-based console redirection only.  
 *** GUI based console redirection.  
 This version does not offer any console redirection services. 
===================================
When connected to the PowerEdge M1000e CMC through HyperTerminal, what command is used to get help on another CMC command?

 *** Help 
 info 
 ?    
 More 
=====================================
What component in the PowerEdge M1000e must be removed prior to removing a network switch module?

 The rack rails 
 The hard-disk drives 
 *** Nothing 
 The front bezel 
===========================================
Which precaution should be taken when replacing PowerEdge M600 or M605 server module processors?

 Remove the DIMM heatsink ===> ´ä¾Æ´Ô
 Allow 10-15 minutes for the blade to cool 
 **** Align the processor key with the slot 
 Remove both processors at the same time 
=======================================
What must be removed before the system board can be removed from the PowerEdge M600 or M605 server modules?

 Hard-disk drive ==> ´ä¾Æ´Ô
 Memory modules ===> ´ä¾Æ´Ô
 Midplane =====> ´ä¾Æ´Ô
 *** System processors  
=====================================

The integrated SAS 6 i/R in the PowerEdge M605 supports Raid 5.

 *** False 
 True 
=======================================
How can a user access the CMC on the PowerEdge M1000e?

 CLI via Null Modem cable ====> Á¤´ä¾Æ´Ô
 CLI via SSH ==> ´ä¾Æ´Ô
 WebUI using a browser  ==> ´ä¾Æ´Ô
 *** CLI via Slot 17 on the iKVM  
===========================================
Which PowerEdge M605 BIOS setting must be disabled to allow Non-Uniform Memory Access?

 Memory Arch Function 
 Uniform Memory Access ==> ´ä¾Æ´Ô
 *** Node Interleaving 
 NUMA 
==============================================
What must be migrated to the new system board during a PowerEdge M600 and M605 system board replacement?

 *** Memory modules.  
 Fibre Channel HBA if present. ==> ´ä¾Æ´Ô
 System processors. ==> ´ä¾Æ´Ô 
 iDRAC. => ´ä¾Æ´Ô
==========================================
When connected to the PowerEdge M1000e CMC through HyperTerminal, what command is used to set the network configuration of the CMC?

 racadm getniccfg  
 *** racadm setniccfg 
 racadm networkcfg  
 racadm autonetwork  
==============================================
A customer reports that he has lost his iDRAC password and does not want to install OMSA, how can this password be recovered?

   The customer must boot to the ASSET utility to replace this password.  
 The customer must replace the system board; this password is not recoverable. 
 The customer must re-flash the system BIOS to recover the password.  
 *** The customer can boot to the CTRL-E option and reset the iDRAC to default.  
=================================================
Which color denotes hot-plug devices on the PowerEdge M1000e?

 Red  
 Blue => ´ä¾Æ´Ô
 Green  => Á¤´ä¾Æ´Ô
 *** Orange 
==============================================
Which color denotes touch points or removable devices on the PowerEdge M1000e?

 Orange ==> ´ä¾Æ´Ô
 Green  ==> ´ä¾Æ´Ô
 Red ==> ´ä¾Æ´Ô
 *** Blue 
================================

What interface options are available for management and configuration of the switch module(PowerConnect 6220) in the PowerEdge M1000e?

 Server Administrator  ==> ´ä¾Æ´Ô
 GUI 
 2161DS Remote Console Switch Software  => ´ä¾Æ´Ô
 ** CLI ?
====================================

The customer purchased a PowerEdge M1000e with a factory install of Windows 2003 server. The customer reports the factory download is corrupt on one of the M600 blades. What are the steps to help the customer resolve this issue?

   Inform the customer that USB CD-ROM peripherals are not supported and that they will need to contact Dell sales to purchase an internal Floppy/CD-ROM module.  
 Call Dell technical support to dispatch a hard drive with the OS pre-installed. 
 **  ? Attach an external USB DVD-drive. Go into system setup and turn USB on with BIOS support. Boot to the CDU CD and the customer can reinstall the OS.  
 Inform the customer that he must purchase a Directline Plus contract and that he should call Dell for assistance after doing so.  

 
The integrated SAS 6 i/R in the PowerEdge M605 supports Raid 5.

==   False 
 True 
