 Multiple Choice: You access the Unified Server Configurator (Lifecycle Controller) and get this message on the welcome screen, "Warning: A system update is recommended since some components are potentially out of date. Please run the update wizard in order to complete this process." What does this message mean? 
 
===Update Driver pack using the Platform update feature in USC, if the Operating System is already installed this update can be performed using a post-OS Dell Update Package. 
 This means the Virtual Flash that plugs in is not up to date. Use this feature to enable or disable vFlash, check the health and properties, and format the vFlash. 
 Boot into the Unified Server Configurator, F10 on P.O.ST.,and select Diagnostics option from the left menu of the USC. Launch the system DMRK diagnostics. 
 The system is in field service mode which means it has been recovered from a corrupt image. Perform Platform Updates via a USB key or FTP repository to bring it back to normal behavior. 


A user can install a Fusion IO (Solid-state PCIe storage card) into the M610x blade.
 ==TRUE
 FLASE

True or False: When you are reinstalling the Fan Cage in the C410x, pressing down on the cage once it is inserted inside the chassis automatically seats the two bottom power connectors.  
  
  False 
 ==True 

When you are reinstalling the Fan Cage in the C410x,pressing down on the cage once it is inserted inside the chassis.....power connectors
==False
  True

Choose All That Apply: M1000e blade chassis PSUs have which of the following indicators?  
 
== Fault indicator 
EMP Pulse indictor 
==AC power source present indicator 
==DC power Indicator 
 
Multiple Choice: What is the rack height for PowerVault 20xS/21xS? 
 
 6U 
 1U 
 4U 
 ==3U 

Choose All That Apply:
Which of the following cables must be disconnected prior to removing the Expander Board from the PowerEdge C1100?  
  
== Power Cable 
Midplane cable 
==Fan cables 
==12C Communication cable 

True/False: The Dell PowerVault LTO5-140HH tape drive offers a formatted cartridge capacity of up to 1500 GB. 
  
  False 
 ==True 
 
 Multiple Choice: What is the maximum possible configuration of hard drives possible on the PowerEdge C6100? 
  
  10 
 12 
 ==24 
 8 
 

Choose All That Apply: M1000e blade chassis supports which of the following generations of Blades Servers? 
 
 
  12th Generation Blades Server 
==10th Generation Blades Server 
==11th Generation Blades Server 
8th Generation Blades Server 
9th Generation Blades Server 

Multiple Choice: Which of the following is NOT an example of Tier 2 or Tier 3 diagnostics? 
  
 PowerEdge Diagnostic 
== Quad pack LEDs 
 Online Diagnostic 
 DSET 
 
 
Choose All That Apply: Which of the following devices must be removed prior to removing the System Board on the PowerEdge C1100?  
 
== Any attached peripherals 
==Cover 
==Power supply 
Hard drives 
 
Multiple Choice: M610x and M610 blades have the same features, EXCEPT for which of the following? 
 
 Max HDD 2 
 Intel Tylersberg 
 ==Support for 2x 16PCIe Slots 
 Support for SAS/SATA/SSD 
 Support RAID 0 and 1 only 
   
 
Multiple Choice: If one of the power connectors are not properly seated when you reinstall the C410x fan cage, you will see multiple Amber fan LEDs and experience a drastic increase in system fan noise when the system is powered ON. 
  
  False 
== True 
 

If you experience all four LEDs on a single side of the C410x fan cage not lit at all, the issue is most likely:  
 
  A damaged fan cage 
== A disconnected or damaged Fan LED cable connector 
 A failed system fan 
 A disconnected fan cage power connector 


 Multiple Choice:
OMSA is reporting that a RAID 6 on a PERC6/i is in a partially-degraded state. What does this mean? 
 
 
  A single drive in the array is partially failed and the array may or may not still be redundant. 
 This is a state somewhere between optimal and failed and the array might still be redundant 
 This is the basically the same as degraded and the array is no longer redundant. 
 ==The array has lost one drive, but is still redundant unless it loses a second drive. 
 
Multiple Choice: On which screen of the BMC the PowerEdge C1100 would you find the Launch VM button to start a Virtual Media session?  
 
 
  System tab 
 Sensors tab 
== Console tab 
 Configuration tab 
 

 Multiple Choice: What is the largest media capacity supported on RD1000? 
 
 
  300GB 
 ==160GB 
 120GB 
 250GB 
 

Choose All That Apply: Select all the key features below which are present on the M610x blade: 
 
 
 == 2 Mezz card slots in expansion blade 
==2 x16 Gen2 PCIe slots with support for x1 to x16 standard PCIe cards 
Half height form factor blade 
==Capability to connect to any 11G or later half height blade 
 
Choose All That Apply: Which versions of Lifecycle Controller include remote services? 
 
 
==Lifecycle Controller 1.4 
==Lifecycle Controller 1.3 
==Lifecycle Controller 1.2 
Lifecycle Controller 1.1 
 
 
  Multiple Choice: The CMC Revision 2.3 firmware in the M1000e blade chassis is able to support which PSU? 
 
 
  1200W PSU 
 ==2360W PSU 
 2700W PSU 
 1350W PSU 

True/False: Recent versions of 'WinDbg' have been distributed as part of the free Debugging Tools for Windows. 
 
 
  False 
== True 

Multiple Choice: DRAC is used to perform which of the following tasks?  
 
 
  Increase the efficiency of the server by administering operations faster 
 Handles the TCP/IP traffic freeing the processor from this task 
 Control the results of specific applications in a server 
 ==Access servers from remote locations independently of the OS status 

Multiple Choice: The PowerEdge R715 Supports the following HDD RAID options using H200 PERC Card, except: 
  
 == Integrated SAS/SATA RAID 5 
 Integrated SAS/SATA RAID 10 
 Integrated SAS/SATA RAID 0 
 Integrated SAS/SATA RAID 1 

Multiple Choice: What is the command used to run PERC 5 configuration utility during system startup stage? 
 
 
  Ctrl C 
 ==Ctrl R 
 Ctrl E 
 Ctrl M 

 True/False:
The PERC 4 controller has a speaker that generates loud warnings when system errors occur. 
 
 
  False 
== True 
 

Multiple Choice: The acronym DRAC stands for : 
 
 
  Dell Remote Application Controller 
== Dell Remote Access Controller 
 Dell Random and Amazing Computing 
 Dell Random Application Computing 
   

 Choose All That Apply: The Lifecycle Controller has which of the possible interfaces described below? 
 
 
  Serial-Over-LAN Proxy (SOL Proxy) ? A telnet daemon that allows LAN-based administration of remote systems using the Serial Over LAN (SOL) and IPMI 1.5 or 2.0 protocols. 
OpenManageServerAdministrator (OMSA) - A comprehensive, one-to-one systems management solution in two ways: from an integrated, Web browser-based graphical user interface (GUI) and from a command line 
===Remote Services ? WS-Management web services interfaces for remote server provisioning and management using iDRAC. 
====Unified Server Configurator (USC) - A graphical UI tool for local access of the Lifecycle Controller features in a pre-OS environment. 
  
 Multiple Choice: On the PowerEdge R410 and T410 servers what is the pre-installed configuration utility that enables systems and storage management tasks from an embedded environment throughout the server¡¯s lifecycle? 
 
 
  Baseboard Management Controller (BMC) 
 HyperV 
=== Dell¢â Unified Server Configurator 
 iDRAC6 
 
On the PowerEdge R905, how many interface cables must be removed from a PERC 6 SAS controller before removing the card?
==2
3
4
1

Which of the following features are supported for DELL EqualLogic "Maintenance"?
==Detailed Historical Performance Monitoring
==Enclosure Monitoring System
==E-mail Home
Auto-Stat Disk Monitoring System
==thin Provisioning


True/False: The PowerVault NX300 NAS system is physically different from the PowerEdge R410 server. 
 
 
  False 
== True 
 

Multiple Choice: Which of the following RAID levels is NOT supported by PERC 5 controller card? 
 
 ===  RAID 6 
 RAID 10 
 RAID 1 
 RAID 50 
 RAID 5 

True/False: If a PCIe x4 or x8 mezz card is required in MEZZ4_FAB_B then a dual PCIe x4 mezz card cannot be used in MEZZ3_FAB_C for M610x blade server. 
 
 
 === True 
 False 
 

Multiple Choice: How can the DRAC 5 be useful to you on a system that will not complete boot?  
 
 
  By providing a system state restore feature, to return the server to the condition it was when it left the factory. 
 There is no way it can be used for troubleshooting a system that is not completing boot. 
==== By providing access to the system event log (SEL) log, and possible last crash screen. 
 By providing a hidden logon screen that allows for the system to phone home with the reason it is failing. 

True/False: PowerEdge Diagnostics test can be used to run test on tape drives. 
 
 
  False 
=== True 

Choose All That Apply: What component can we find in the rear of M1000e blade chassis? 
 
 
==  6 x Power Supply Units 
==1 x iKVM (optional device) 
===9 x Fan Modules 
None of the above 
===6 x I/O Modules (IOMs) 

 True/False: PowerEdge Diagnostic tool is only available for installation on Windows platform. 
 
 
  True 
 ==False 
 

True/False: The mixing of 1350W (110VAC) and the 2360W/2700W (220VAC) is NOT allowed in the M1000e blade chassis. 
 
 
  False 
=== True 
 

True/False: The PowerEdge T110 has a redundant power supply that will automatically switch to the closest voltage that matches the AC power available at customer location. 
 
 
  True 
=== False 

Choose All That Apply: Which of the following components must be removed first from the PowerEdge T105 before removing the system board? 
 
 
 ==Power cord 
Power supply 
==Computer cover 
==Processor 

Choose All That Apply: On the PowerEdge C6100, where is the power button for Motherboard 1 located?  
 
 
  As one of four numbered power buttons on a control panel at the right side of the front of the chassis 
As one of four labeled power buttons next to the power supplies in the rear of the system. 
====The top power button (of two) on the left side control panel on the front of the chassis. 
====On the right hand corner of the node when viewed from the rear of the system 


Multiple Choice: DRAC helps the customer save money by:  
 
 
  Managing more applications simultaneously 
 ==Enabling the customer to manage and monitor multiple systems at possibly multiple locations from a single location without travelling from location to location. 
 Handling more tasks at the same time 
 Creating a virtual server within the main server. 
 

Multiple Choice: What interface is used by the connectors on the back panel on the PowerVault 220S/221S? 
 
 
  SAS 
 USB 
=== SCSI 68-pin 
 SATA 

Choose All That Apply: DSET can be used to gather which of the following information? 
 
 
 == PERC controllers information such as controller logs, information and firmware level 
==Operating systems information such as event log, stop error codes and driver information 
System backup job log 
==Dell server's service tag 
  

Multiple Choice: Which component is faulty if the PowerEdge R200 displays a yellow-yellow-green-yellow diagnostic LED code? 
 
 
  Memory 
 System board 
=== Processor 
 Video card 

Choose All That Apply: Which of the following optional storage controllers does the R300 support? 
 
 
  PERC 6 RAID 
==SAS 6 iR 
==SAS PERC 5/E 
PERC 4 
==SAS 6 
  

True/False: "Windbg" is usually used for debugging kernel-mode memory dumps created after what is commonly called the Blue Screen of Death. 
 
 
  ===True 
 False 

Choose All That Apply: Which of the following statements are true regarding a Tier 1 diagnostic tool? 
 
 
 ==== Is built into PowerEdge and PowerEdge SC firmware 
=====Can provide diagnostic information about the machine 
====Gives codes you can research for their meaning and corrective actions 
=====Does not require any additional software or hardware 
=====Is always available as long as the server is powered up 

True/False: It is not necessary to power the C410x chassis OFF before removing one of the GPU cages. 
 
 
 === False 
 True 


How do you enter the DRAC configuration utility for 9th, 10th & 11th server generation systems? 
 
 
  CTRL + D 
 CTRL + S 
 ==CTRL + E 
 CTRL + H 


 Multiple Choice: A customer has a PowerEdge T605 with two processors and eight 1GB DIMMs installed and memory sparing is turned on in the system BIOS. What is the total amount of available memory on the system when configured in this manner? 
 
 
 === 4GB 
 8GB 
 1GB 
 2GB 
 

Multiple Choice: What is the maximum amount of hard drives possible on the PowerEdge C1100?  
 
 
  8 
 ===10 
 12 
 24 
 

 Multiple Choice: The M610x blade server uses the same system board as: 
 
 
  M910 
 M610 
 M805 
 R610 
===== M710 

 Multiple Choice: Which of the following is true of PERC 6 support for SATA drives? 
 
 
 ===== SATA drives are supported by the PERC6, but may not be mixed in virtual disks with SAS drives. 
 SATA drives are supported by the PERC6 and may be mixed in virtual disks with SAS drives. 
 The PERC6 does not support SATA drives; it only supports SAS drives. 
 

Choose All That Apply: Which of the following devices must be removed prior to removing the C410x Fan Cage? 
 
 
===  Back Cover 
==Middle Cover 
==All System Fans 
Middle board 

Multiple Choice: Which of the following statements is true regarding plugging the C410x enclosure into a 110V power source and powering it ON?  
 
 
  The system will POST and the system fans will all spin up, but you will receive an error code on the LCD screen. 
 The system will not even show any signs of attempting to power ON. 
 The system will power ON completely and function, but only with a maximum of 4 GPUs installed. 
==== The system power button will illuminate, but the system will not completely power ON and none of the system fans will spin up. 

 Multiple Choice: You access the Unified Server Configurator (Lifecycle Controller) and get this message on the welcome screen, "Warning: A system update is recommended since some components are potentially out of date. Please run the update wizard in order to complete this process." What does this message mean? 
 
 
  The system is in field service mode which means it has been recovered from a corrupt image. Perform Platform Updates via a USB key or FTP repository to bring it back to normal behavior. 
 This means the Virtual Flash that plugs in is not up to date. Use this feature to enable or disable vFlash, check the health and properties, and format the vFlash. 
== Update Driver pack using the Platform update feature in USC, if the Operating System is already installed this update can be performed using a post-OS Dell Update Package. 
 Boot into the Unified Server Configurator, F10 on P.O.ST.,and select Diagnostics option from the left menu of the USC. Launch the system DMRK diagnostics. 


 True/False: The M610x blade is able to support the NVIDIA Tesla GPU card. 
 
 
  False 
 ====True 

Multiple Choice: What is the external interface for the PowerVault RD1000? 
 
 
  iSCSI 
 SCSI 
 SAS 
 =====USB 

 True/False: The green dual-bus indicator (middle) lights when the PowerVault 2xxS is operating in dual-bus split backplane mode.  
 
 
  False 
 ===True 

Multiple Choice: Which of the following fabric options is NOT supported in the M1000e Blades Chassis? 
 
 
  PowerConnect M8024 10Gb Ethernet Switch (SFP+, CX4, & 10Gbase-T uplink module options) 
 10Gb Ethernet Pass-Through Module (SFP+) 
 PowerConnect M6220 Switch; GbE + 10GbE uplinks & stacking 
 ===PowerConnect 8800 Rackmount Switch 
 PowerConnect M6348 Switch; 48 1GbE ports + 10GbE uplinks 

 True/False: Disk migration of PERC 5 SAS RAID controllers is supported within the PERC 5 family only. The PERC 5 SAS RAID controllers are not backward compatible with previous PERC RAID controllers.  
 
 
====  True 
 False 

Multiple Choice: Which of the following sizes of TORX drivers are listed as preferred in the toolkit? 
 
 
  T5, T7, T10, T11 
 T3, T5, T7, T9 
 T6, T7, T8, T9 
==== T8, T10, T15, T20 
   
 
 
 
 
 

 

 

 
 

 
 
 

 
 

 

 
 
 

 
 
 

 

 
 
 

 
 
 
