The Storage Management Command Line Interface (SMcli) in interactive mode has complete error checking and will give the user useful feedback during use.

=   False 
 True 


What is the new term for channel on a PowerVault MD1000 with a PERC5/e?

=   Connector 
 Sub-channel 
 Port 
 Field 


If an administrator password is set on a PowerVault MD3000, configuration change commands can still be issued from the Storage Management Command Line Interface (SMcli).

?  True 
 False 


When replacing the backplane in a PowerVault MD3000, although it is recommended to replace the service tag on the new backplane with the original service tag, the Premium Features will continue to operate normally with the new service tag. 

   True 
=?? False 



When using the Storage Management Command Line Interface (SMcli), it is recommended to use the interactive interface rather than the scripted interface.

=   False 
 True 


What is the maximum allowable cable length when connecting SAS on the PowerVault MD3000?

   6 meters 
 12 meters  
 1 meter  
= 4 meters 


What common color is the front drive carrier on the PowerVault MD3000?

   Gold  
 Blue  
 Terracotta  
= Black  


In a PowerVault MD3000 with single port controllers, only one Host can be connected.

=   True 
 False 



In a PowerVault MD3000 with dual port controllers, each Host will have both of its HBAs cabled to one controller.

=   False 
 True 



How many captive screws secure the battery assembly in the RAID Controller Module of the PowerVault MD3000?

   3 
= 2 
 0 
 1 


How many hard drives are supported in the PowerVault MD3000 storage enclosure?

=   15 
 14 
 18 
 16 


In cabling each host to the PowerVault MD3000, each host must have a minimum of two SAS connections to the Storage Array.

   True 
= False 




How many power cables are required to plug-in the two power supplies on the PowerVault MD3000?

=   2 
 1 
 0 
 7 
Even if a PowerVault MD3000 power supply fails, the enclosed fans will continue to operate on the common fan bus voltage bus.

=   True 
 False 


Each PowerVault MD1000 power supply is secured with three thumbscrews.

   True 
= False 




If a power supply/cooling fan module fails in a PowerVault MD3000, which of the following is the most accurate?

   The fans in the failed module will not continue to operate but the failed module must be left in place. 

?? The fans in the failed supply will continue to operate until the module can be replaced 

 The module must be removed, even if a replacement is not available. 

 The fans in the failed supply will come on only if the enclosure temperature reaches the ¡°critical¡± set point. 

 
Each PowerVault MD3000 power supply is secured with three thumbscrews.

   True 
= False 


If a PowerVault MD3000 hard drive is accidentally removed while the drive is online how long should the user wait before re-inserting the drive?

   5 minutes  
 No waiting is necessary  
= 30 seconds  
 10 seconds 


How many screws secure the front faceplate on a PowerVault MD3000?

   10 
 14 
= 16 
 18 


What type of drives are supported in the PowerVault MD3000? 

   Floppy  
 None of those listed  
 IDE  
= SAS hard drives  


How many screws must be removed from the EMM/power supply cage when removing the PowerVault MD3000 midplane?

   8 
 6 
= 4 
 16 

True/False 
In a PowerVault MD3000 with dual port controllers, each Host will have both of its HBAs cabled to one controller.

==   False 
 True 




True/False 
Even if a PowerVault MD3000 power supply fails, the enclosed fans will continue to operate on the common fan bus voltage bus.

   False 
=== True 

