What additional device must be performed after removing the system board assembly on a C6100 before you can remove the memory DIMMs from the system board? 

   Hard drives  
 Heat sink  
= Cooling shroud  
 Cooling fans  

Each Node (system board assembly) in the PowerEdge C6100 chassis has a single NIC and a single dedicated 'KVM over IP' BMC connection integrated on its system board. 

=   TRUE 
 FALSE 

What is the maximum amount of memory possible on a fully populated PowerEdge C6100 per node (system board assembly) installed? 

   192GB 
 48GB 
= 96GB 
 72GB 

Which of the following devices must be removed before removing the system board from the system board assembly on a C6100? 

=   Memory DIMMs  
 Hard Disks  
= Processor  
= Heat sink  

The PowerEdge C6100 supports Memory Mirroring. 

   TRUE 
= FALSE 

The PowerEdge C6100 fans are all removed together as an assembly. 

=   TRUE 
 FALSE 

The PowerEdge C6100 system board assemblies are commonly referred to as Nodes. 

=   TRUE 
 FALSE 


What is the function of the backplane jumper labeled 'A' on the C6100? 

   LED Control  
= Hard Drive Type Select  
 MFG Test  
 SAS Code Select  

On the PowerEdge C6100 where can you find a power button for Server Node 1? 

   As one of four labeled power buttons next to the power supplies in the rear of the system.  
 As one of four numbered power buttons on a control panel at the right side of the front of the chassis.  
= The top power button (of two) on the left side control panel on the front of the chassis.  
=On the right hand corner of the node when viewed from the rear of the system.  

If you install only a single CPU in a node to test the CPU socket for minimum POST functionality, what video message will be displayed? 

=   Unsupported CPU combination. System Halted!  
 Incorrect CPU configuration  
 Missing CPU 1  
 Missing CPU 2  


Choose All That Apply:
Which of the following must be removed before removing a Power Distribution Board on the PowerEdge C6100? 

 =  Cover  
 =Power Supplies  
 = Securing screws  
 All Hard Drives  

What is the maximum amount of hard drives possible on the PowerEdge C6100? 

  == 24 
 8 
 12 
 10


