Dell OpenManage Server Assistant helps users install a server operating system.

   False 
= True 


If a RAID controller is installed in a server when it is booted with the DSA CD, an option will be appear to configure RAID on the system.

   False 
= True 


The DSA CD can be used to install Red Hat Linux on a server.

=   True 
 False 


RAID 5 combines striping of a RAID 0 with an exclusive OR operation to calculate recovery data.

   False 
= True 


Dell's RAID controllers support the following levels:

=   0 
= 1 
= 50 
 30 


The XEON CPU in the PowerEdge 6800/6850 is different from the XEON MP which is:

=   Designed to run on more than two CPUs 
 Less on-die cache 
 An upgrade to the older MX technology 
 Designed to run on only one CPU 


Virtual disks can be created using a Dell PERC 4/di controller.

=   True 
 False 

The BMC firmware on a PE850 can be updated via a USB memory key.

=   True 
 False 

Data is duplicated at a block level in RAID 1 to create ________ identical drives.

   5 
= 2 
 7 
 3 

Which network card is integrated on the PowerEdge 850 system board?

   Broadcom BCM5704 
 Intel 82450 
 Intel 83451E1 
= Broadcom 5721J 

Which RAID controllers are supported on the PowerEdge 830?

=   PERC4e/DC 
 PERC4/DC 
= CERC SATA 6ch 
= PERC4/SC 

Which memory module is not supported on the PowerEdge 850?

   1 GB DDR2 667 MHz unbuffered SDRAM DIMM  
= 256 MB DDR2 400 MHz unbuffered SDRAM DIMM  
 512 MB DDR2 533 MHz unbuffered SDRAM DIMM  
 2 GB DDR2 667 MHz unbuffered SDRAM DIMM  


Memory must be installed as follows in the PowerEdge 6850:

   In pairs (single-rank only) 
 Both banks per riser card 
 Every other slot on the riser card 
= In pairs (ranks must match within the bank) 


Spare bank and memory mirroring can be enabled at the same time on the PowerEdge 6850.

=   False 
 True 


The PowerEdge 6850 has a dedicated slot for an Integrated Fibre Channel Module.

   False 
= True 



The PowerEdge 6800 and PowerEdge 6850 uses a Xeon MP processor.

=   False 
 True !!!


Which of the following expansion slots are available in the PowerEdge 6850?

=   PCI-e and PCI-x 
 PCI-x only 
 PCI-e only 
 AGP and PCI-e 

The PowerEdge 6800/6850 features Memory RAID technology.

=   True 
 False 

The BMC firmware on a PE850 can be updated via a USB memory key.

   False 
= True 

BMC Firmware installation is supported under the following operating systems:

= Windows 2000 
= Windows Server 2003 
  HP Unix  
= Red Hat Enterprise Linux 3 i386 


With Dell OpenManage Array Manager 2.5 or later installed, DSET gathers information on:

=   Enclosures 
 SDRAM memory 
= PERC controllers 
= Array/containers 

The ESM log can be cleared using the DSET utility.

=   True 
 False 

Which of the following PowerEdge system board firmware can be updated within Windows 2003?

=   BIOS 
 Modem 
= ESM 
= BMC 


BIOS on a Dell system can be updated from the following devices:

=   Diskette 
= USB memory key 
= Flash memory chip 
= CD-ROM 


In which section of the system setup of the PowerEdge 830 would you ensure that the diskette drive is the first boot device?

=   Boot sequence 
 Diskette Drive under Integrated Devices 
 System boot 
 Drives 


Which component is not required to complete POST on the PowerEdge 830?

=   Hard-disk drive 
 Memory 
 System board 
 Processor 

The PowerEdge 6850 has a media bay that accepts two additional hard-disk drives.

   True 
= False 

Which of the following FRUs are offered as hot pluggable in the PowerEdge 6800?

   Memory riser boards 
= System fans 
= Power supplies 
= Hard-disk drives 

The PowerEdge SC430 supports operating system based RAID 0 and RAID 1.

=   True 
 False 

How many USB ports are on the front of the PowerEdge SC430?

   4 
 0 
 1 
= 2 


When using the SC RAID Manager software, which RAID controllers are supported ?

   PERC 4/DC 
= Adaptec 39320 
= CERC SATA 6ch 
= CERC SATA 2s 


Which service must be set to Automatic in order to enable CD-R/CD-RW recording in Microsoft Windows Server 2003 on the PowerEdge SC430?

   CDR/CDRW Logical Disk Manager 
 Distributed Transaction Coordinator 
= IMAPI CD-Burning COM 
 Background Intelligent Transfer Service 

Which of the following PowerEdge SC430 replacement components ship with heat sink grease when being replaced?

   Hard-disk drive 
= Processor fan 
= Bezel 
 =Power Supply 

Dell OpenManage Server Assistant helps users install a server operating system.

   False 
= True 

The DSA CD can be used to install Red Hat Linux on a server.

=   True 
 False 

The Dell Server Assistant (DSA) CD-ROM provides the following:

=   System configuration 
= Installation support 
= Device drivers 
 Server performance ratings 

Virtual disks can be created using a Dell PERC 4/di controller.

=   True 
 False 

Dell's RAID controllers support the following levels:

=   0 
 30 
= 50 
= 1 



Which memory module is not supported on the PowerEdge 850?

=   256 MB DDR2 400 MHz unbuffered SDRAM DIMM  
 512 MB DDR2 533 MHz unbuffered SDRAM DIMM  
 1 GB DDR2 667 MHz unbuffered SDRAM DIMM  
 2 GB DDR2 667 MHz unbuffered SDRAM DIMM  


Which video controller is integrated on the system board of the PowerEdge 830?

=   XGI XG20 PCI 
 No video controller is inetgrated - a PCI card is used 
 ATI Radeon 7000-M 
 ATI Rage XL 


Which component is faulty if the PowerEdge 830 displays a yellow-yellow-green-yellow diagnostic LED code?

   System board 
 Video card 
 Memory 
= Processor 

Spare bank and memory mirroring can be enabled at the same time on the PowerEdge 6850.

=   False 
 True 


Memory must be installed as follows in the PowerEdge 6850:

   Every other slot on the riser card 
 In pairs (single-rank only) 
 Both banks per riser card 
= In pairs (ranks must match within the bank) 


The PowerEdge 6850 has a dedicated slot for an Integrated Fibre Channel Module.

=   True 
 False 


The PowerEdge 6800/6850 features Memory RAID technology.

   False 
= True 



Demand Based Switching (DBS) on the PowerEdge 6800/6850 is designed to achieve: 

   Better I/O bus resource management 
= Reduced power consumption 
 Faster switching between tasks 
 Better use of memory 

Memory size may be increased dynamically at run-time using the hot add capability of the chipset on the PowerEdge 6850 when the following conditions are met:

   Supported OS and empty memory slots in the riser 
 System power must be turned off and open riser slots must be available 
 OS independent and open slots on the riser 
= Supported OS and existing empty riser slot 



BMC Firmware installation is supported under the following operating systems:

=   Red Hat Enterprise Linux 3 i386 
 HP Unix  
 Windows 2000 
= Windows Server 2003 





With Dell OpenManage Array Manager 2.5 or later installed, DSET gathers information on:

=   Array/containers 
= PERC controllers 
= Enclosures 
 SDRAM memory 


The ESM log can be cleared using the DSET utility.

   False 
= True 


BIOS on a Dell system can be updated from the following devices:

=   USB memory key 
= Diskette 
= Flash memory chip 
= CD-ROM 


The system BIOS on a PowerEdge Server can be updated within Red Hat.

=   True 
 False 


What is the first step in the EasyExchange process on the PowerEdge 830?

   Disconnect the SCSI cable from the drive 
 Remove the side cover 
= Turn the system power off 
 Remove the bezel 


How tall is the PowerEdge 850?

=   1U 
 2U 
 5U 
 7U 


Which of the following FRUs are hot-pluggable in the PowerEdge 6850?

=   Power supplies 
= Memory riser boards 
= PCI-e 
 Floppy/CDROM combo 


Which of the following FRUs are offered as hot pluggable in the PowerEdge 6800?

   Memory riser boards 
= Hard-disk drives 
= System fans 
= Power supplies 


How many USB ports are on the front of the PowerEdge SC430?

=   2 
 0 
 4 
 1 


Which of the following PCI-e slot options are available in the PowerEdge SC430?

=   X8 PCI-e slot linked at X4 speed 
  X16 PCI-e slot linked at X8 speed 
= X1 PCI-e slot 
 X4 PCI-e slot 


When using the SC RAID Manager software, which RAID controllers are supported ?

   PERC 4/DC 
= CERC SATA 6ch 
= CERC SATA 2s 
= Adaptec 39320 


A customer has a PowerEdge SC430 system that will not POST and is displaying a 1-4 diagnostic LED code. What is most likely the faulty component?

=   System board 
 Processor 
 Memory 
 Hard disk 


To remove the front system fan in a PowerEdge SC430, you must first remove which components:

   System board 
= Cover 
= AC Power cable 
= Heatsink 



A customer has a PowerEdge SC430 system that will not POST and is displaying a 3-4 diagnostic LED code. What is most likely the faulty component?!!!

   Processor 
 System board 
= Memory ~~p
 Hard-disk driv



Memory is only hot-plugged in the PowerEdge 6850 when:

   A redundant memory configuration is active 
 A spare blank is active 
 The system is powered off 
= Only RAID memory is active 


The Dell Smart USB flash drive can be made a bootable device.

=   True 
 False 


An additional PCI SCSI/RAID controller is required to support the 1x10 + 1x2 hard-disk drive configuration on the PowerEdge 6800.

   True 
= False 

RAID Management utilities that provide error statistics logging are

dell open array manager
bios
linux


The BMC firmware on a PE850 can be updated via a USB memory key

true

DSET is a small intrusive tool that does not require reboot of the system.
true



)