How many power cables are required to plug-in the two power supplies on the PowerVault MD1000?

   7 
= 2 
 1 
 0 

Each PowerVault MD1000 power supply is secured with three thumbscrews.

   True 
= False 


??An Array Disk in the PowerVault MD1000 is annotated in the following format:

   Port:enclosure:slot 
? Connector:enclosure:slot 
 Connector:enclosure:port 
 Controller:connector:slot 



What keystroke(s) are used on BOOT of the to access the PowerVault MD1000 BIOS level interface on the PERC5/E?

=   Ctrl + R 
 Ctrl + P 
 ALT + P 
 ALT + R 


What type of drives are supported in the PowerVault MD1000 SAS Enclosure?

   Floppy 
= SAS hard drives 
 IDE 
 None of those listed 



How many screws must be removed from the EMM/power supply cage when removing the PowerVault MD1000 midplane? 

   6 
= 4 
 16 
 8 


When viewing the PowerVault MD1000 from the back, the primary power supply module is located on the left side. 

   False 
= True 



What common color is the front drive carrier on the PowerVault MD1000?

   Blue 
 Terracotta 
 Gold 
= Black 


?What is the new term for channel on a PowerVault MD1000 with a PERC5/e?

   Sub-channel 
= Port 
 Field 
 Connector 


How many hard drives are supported in the PowerVault MD1000 storage enclosure?

   14 
 12 
 16 
= 15 



What is the maximum allowable cable length when connecting SAS on the PowerVault MD1000?

   1 meter 
= 4 meters 
 12 meters 
 6 meters 

In the PowerVault MD1000 BIOS PERC5/E interface, what keystroke(s) access the next page?

 =  CTRL + N 
 Ctrl + R 
 Ctrl + P 
 Alt + P 


How many screws secure the front faceplate on a PowerVault MD1000?

   18 
 10 
= 16 
 12 



What type of drives are supported in the PowerVault MD1000 SAS Enclosure?

   IDE 
 Floppy 
= SAS hard drives 
 None of those listed 


