Servers - PowerEdge 600SC Product Certification (15 Questions)

True/False:
To remove the front bezel on the PowerEdge 600SC, press the blue tabs towards the front of the chassis.
True.
False.

True/False:
To remove the front fan in the PowerEdge 600SC, you must loosen the two thumbscrews that secure the front fan to the chassis?
False.
True.

Multiple Choice:
On the PowerEdge 600SC, what FRU is the processor fan cable connected to?
The system board.
The hard drive.
The chassis.
The front bezel.

True/False:
There are six screws that secure the power supply to the chassis.
True.
False.

True/False:
When removing a hard-disk drive from the PowerEdge 600SC, press the hard-disk drive cage tab to pull the hard-disk drive cage away from the chassis.
False.
True.

True/False:
On the PowerEdge 600SC, you must pinch the two slide rail assemblies together to remove the CD-ROM drive from the chassis.
True.
False.

True/False:
On the PowerEdge 600SC, you must remove the two screws securing the floppy-disk drive to the chassis.
True.
False.

True/False:
On the PowerEdge 600SC, you must pull the control panel off the plastic retaining clips in order to remove the control panel from the system.
True.
False.

Multiple Choice:
In the PowerEdge 600SC, where must you slide the system board in order to remove it?
Towards the front of the chassis.
Towards the bottom of the system chassis.
Towards the back of the system chassis.
Towards the top of the system chassis.

True/False:
To remove the processor in the PowerEdge 600SC, you must disconnect the heat sink fan cable from the power supply.
False.
True.

Multiple Choice:
On the PowerEdge 600SC, how many heat sink retention arms secure the processor heat sink to the ZIF socket?
One.
Four.
Three.
Two.

Choose all that apply:
On the PowerEdge 600SC, what must be performed prior to removing the memory?
Disconnect the AC power cable from the back of the system.
Remove the system board.
Remove the processor fan.
Open the cover.

Multiple Choice:
What is the maximum number of processors that the PowerEdge 600SC will support?
One.
Four.
Two.
Three.

Multiple Choice:
What is the maximum number of PCI cards that can be installed in the PowerEdge 600SC?
Two.
Three.
Four.
Five.

Multiple Choice:
How many channels does the embedded IDE controller contain in the PowerEdge 600SC contain?
Three.
Five.
One.
Seven.