Multiple choice:
To remove the hard drives on the PowerVault 210S/211S, which one of the following components must first be removed
The hard drive fan assembly
The hard drive locking bar
The ES module
The power cabling harness

Multiple choice:
What is the maximum speed supported by the internal SCSI controller in the PowerEdge 1550
80MB
160MB
20MB
40MB

Multiple Choice:
On the PowerEdge 1650, where is the fan bracket release located
Next to the control panel.
Next to the front power supply
Next to the CD-ROM drive
Next to the PCI riser board

Choose all that apply:
In the PowerEdge 1650, What must be done before removing the floppy-diskette drive cable.
Open the top panels
Press the metal tab next to the front power supply
Remove the front bezel
Pull the ZIF connector up.

True/False:
To replace the back power supply on the PowerEdge 1650, slide the back power supply towards the front of the system.
True
False

Multiple Choice:
On the PowerEdge 1650, what secures the system board to the chassis?
A solder joint
A metal clamp
Retaining clips
A thumbscrew

Multiple Choice:
What RAID option is available for the internal SCSI drives on the PowerEdge 1650
PERC 3/DI
PERC 3/DC
PERC 3/DCL
PERC 3/SI

True/False:
A PowerEdge 1650 configured with IDE hard-disk drives will not contain a hard-disk drive backplane
True
False

True/False:
On the PowerEdge 2550, empty processor sockets are required to be filled with a terminator card.
True
False

Multiple Choice:
The PowerEdge 2600 contains how many memory module sockets?
12
6
10
8

Multiple Choice:
What is the maximum number of Xeon processors that the PowerEdge 2600 will support?
Four
Two
Three
One

True/False:
On the PowerEdge 2600, the ROMB memory module socket is grouped together with the system memory module sockets
True
False

Multiple Choice:
On the PowerEdge 2600, where are the three thumbscrews located that secure the system cover to the chassis
On the front of the system
On the left side of the system
On the right side of the system
On the back of the system

True/False:
On the PowerEdge 2600, the PCI slot guide assembly must be removed to be able to remove the ERA.
False
True

Multiple Choice:
What FRU is the split backplane card plugged into on the PowerEdge 2600
The PDB
The ROMB hardware
The peripheral bay backplane
The backplane

Multiple Choice:
What color latches on the slide rail assembly must you lift up to allow you to push the PowerEdge 2650 into a rack

You have 134 minutes left (as of the time this page was requested from the server).

Microsoft VBScript runtime error '800a000d'

Type mismatch: 'cInt'

/Member/ShowTest.asp, line 180

(Happened on 5:34PM Friday, 21 March 2003)