Question # 30 of 30

You have 99 minutes left (as of the time this page was requested from the server).

Multiple Choice 
Which of the following PV136T LTO Library components provides fibre channel to SCSI connectivity?

   Main PCBA. 
 RMU. 
 SCSI Host Interface PCBA. 
 FC Bridge. ***

Question # 29 of 30

You have 102 minutes left (as of the time this page was requested from the server).

Multiple Choice 
When an error occurs in the PV136T LTO Library, the information displayed on the operator panel is a:

   Fault Symptom Code (FSC) code. 
 Fault code. 
 Service Action Code (SAC) code. ****
 ERR code. 

Question # 28 of 30

You have 102 minutes left (as of the time this page was requested from the server).

Multiple Choice
The PV136T LTO Library automates the retrieval, storage, and control of the following tape cartridges:

   TR5. 
 LTO. ***
 DLT. 
 SDLT. 

Question # 27 of 30

You have 102 minutes left (as of the time this page was requested from the server).

Multiple Choice 
The SCSI interface to the PV136T LTO Library is:

   IDE. 
 SCSI2. 
 LVD. ****
 HVD. 

Question # 26 of 30

You have 102 minutes left (as of the time this page was requested from the server).

Multiple Choice 
A PV136T LTO Library with four columns and a locked multiple slot mailbox can store a maximum of ________ tape cartridges:

   60. 
 42. 
 72. ***
 24. 

Question # 25 of 30

You have 103 minutes left (as of the time this page was requested from the server).

Multiple Choice 
The Y-Axis motor is mounted to the PV136T LTO Library chassis with:

   A Y-Axis belt loop. 
 Two T20 Torx screws. *****
 One cable clamp. 
 Two T8 Torx screws. 


Question # 24 of 30

You have 103 minutes left (as of the time this page was requested from the server).

Multiple Choice 
How many nuts must be loosened on the belt tension mechanism first before loosening the tension on the Y-Axis belt in the PV136T LTO Library?

   One. 
 Four. 
 Eight. 
 Three. *

Question # 23 of 30

You have 104 minutes left (as of the time this page was requested from the server).

Choose all that Apply
Use the following tools to remove the Y-Axis drive belt in the PV136T LTO Library:

   Flashlight. ***
 T8 Torx driver. ***
 3/16 inch nut driver. ***
 11/32 open-end  


Question # 22 of 30

You have 104 minutes left (as of the time this page was requested from the server).

Choose all that Apply
Remove the following FRUs from the PV136T LTO Library before removing the Y-Axis drive belt:

   Plastic lower grill. 
 Top cover. ***
 Power supplies. ***
 Tape drive modules. *** 

Question # 21 of 30

You have 104 minutes left (as of the time this page was requested from the server).

Multiple Choice 
Column three in the PV136T LTO Library contains:

   One fixed tape slot. 
 Three tape storage magazines. 
 A mailbox. 
 Tape drive modules. ***

Question # 20 of 30

You have 105 minutes left (as of the time this page was requested from the server).

Choose all that Apply
Storage Column Two in the PV136T LTO Library is secured to the chassis with:

   One 7/16 inch bolt. ***
 Two 7/16 inch bolts.  
 Two T20 Torx screws. ***
 Two T8 Screws. 

Question # 19 of 30

You have 105 minutes left (as of the time this page was requested from the server).

Multiple Choice 
The power distribution PCBA in the PV136T LTO Library is secured to the chassis by:

   Four T8 Torx screws. 
 The AC input module. 
 Four 11/32 inch nuts. ***
 The tape drive module power cables. 


Question # 18 of 30

You have 105 minutes left (as of the time this page was requested from the server).

Multiple Choice 
The power distribution PCBA in the PV136T LTO Library is secured to its metal frame with:

   One Phillips-head screw. 
 Seven T8 Torx screws. 
 Four 11/32 inch nuts. 
 Seven Phillips-head screws. ***

Question # 17 of 30

You have 107 minutes left (as of the time this page was requested from the server).

Multiple Choice 
Before removing the picker control PCBA from the PV136T LTO Library, first:

   Remove storage column 2. ***
 Set the main power switch to on. 
 Remove the picker assembly. 
 Remove the power distribution PCBA. 

Question # 16 of 30

You have 108 minutes left (as of the time this page was requested from the server).

Multiple Choice 
During removal of the picker control PCBA in the PV136T LTO Library, the picker assembly is supported high on the Y-shaft by:

   A scratch tape in column 2. 
 A scratch tape in column 4. ***
 A 12 inch piece of styrofoam. 
 Two T8 Torx screws. 

Question # 15 of 30

You have 108 minutes left (as of the time this page was requested from the server).

Choose all that Apply
The tools required to remove and replace the picker assembly in the PV136T LTO Library are:

   Black marker pen. ***
 11/32 inch open-end wrench. 
 Flashlight. ***
 T20 Torx driver. ***


Question # 14 of 30

You have 108 minutes left (as of the time this page was requested from the server).

Multiple Choice
When replacing the picker assembly on the PV136T LTO Library, the top ground wire connector must be:

   Removed. 
 Positioned vertically. 
 Positioned horizontally. ***
 Connected to storage column 2. 

Question # 13 of 30

You have 109 minutes left (as of the time this page was requested from the server).

Choose all that apply
Remove the following FRUs first before removing the display panel flex cable in the PV136T LTO Library:

   Plastic lower grill. ***
 Tape column 4. 
 Tape drive modules. *** 
 Power Supplies ***

Question # 12 of 30

You have 109 minutes left (as of the time this page was requested from the server).

Choose all that Apply
The tools required to remove the display panel flex cable on the PV136T LTO Library are:

   Flashlight. ***
 11/32 inch open-end wrench. ***
 Flat-blade screwdriver. 
 T8 Torx driver. ***

Question # 11 of 30

You have 111 minutes left (as of the time this page was requested from the server).

Choose all that Apply
Before installing Windows 2000 drivers in the server attached to the PV136T LTO Library, do the following first:

   Verify SCSI controller drivers are installed.  ***
 Load a tape cartridge in a tape drive. 
 View the tape drives during POST. ***
 Attach the server to the FC bridge. 

Question # 10 of 30

You have 112 minutes left (as of the time this page was requested from the server).

Multiple Choice 
To reach the cable clamps that secure the Y-Axis flex cable to the top of the PV136T LTO Library chassis, remove:

   The main controller PCBA mounting bracket. ***
 Storage column four. 
 The plastic top door. 
 Teh plastic lower grill 

Question # 9 of 30

You have 112 minutes left (as of the time this page was requested from the server).

Choose all that apply
Before removing a tape drive module from the PV136T LTO Library, first remove:

   Handle.  
 SCSI cables. ***
 Power Distribution PCBA. 
 AC power cord. 

Question # 8 of 30

You have 113 minutes left (as of the time this page was requested from the server).

True/False 
In the PV136T LTO Library, the FC bridge must be removed first before removing the RMU.

   True. 
 False. ***

Question # 7 of 30

You have 117 minutes left (as of the time this page was requested from the server).

Multiple Choice 
The main controller PCBA support bracket in the PV136T LTO Library must be removed to:

   Gain access to the serial cable. 
 Gain access to the main controller serial cable clamps. ***
 Remove the main PCBA. 
 Gain access to the power distribution PCBA. 

Question # 6 of 30

You have 117 minutes left (as of the time this page was requested from the server).

Multiple Choice 
The main controller PCBA is secured to the PV136T LTO Library with:

   The SCSI host interface PCBA. 
 One T8 Torx screw. ***
 A clamp. 
 Two T8 Torx screws. 

Question # 5 of 30

You have 118 minutes left (as of the time this page was requested from the server).

Multiple Choice 
First do the following before removing the multiple slot mailbox assembly from the PV136T LTO Library:

   Remove the power supplies. 
 Open the tape library front door. ***
 Remove the plastic top door. 
 Remove the tape drive modules. 

Question # 4 of 30

You have 118 minutes left (as of the time this page was requested from the server).

Multiple Choice 
Which of the following tools is needed to remove the FC bridge in the PV136T LTO Library?

   Flat-blade screwdriver. ***
 11/32 inch nut driver. 
 Phillips-head screwdriver. 
 T20 Torx driver. 

Question # 3 of 30

You have 118 minutes left (as of the time this page was requested from the server).

Multiple Choice
The display panel on the PV136T LTO Library is secured with:

   Four Phillips-head screws. 
 The mailbox cable harness. 
 Six Phillips-head screws. ***
 Six T8 Torx screws. 

Question # 2 of 30

You have 120 minutes left (as of the time this page was requested from the server).

Multiple Choice 
The AC input module is secured to the PV136T LTO Library chassis with:

   An AC cable connector. 
 A connector at the back of the AC input module. 
 Two Phillips-head screws. 
 Two T8 torx screws. ***

Question # 1 of 30

You have 120 minutes left (as of the time this page was requested from the server).

True/False
The PV136T LTO Library will operate with only one power supply.

   True. ***
 False. 



=========================================================


After replacing the FC bridge in the PV136T LTO Library, you must:

   Load the mailbox. 
 Setup the same configuration of the previous FC bridge. **
 Attach the power cord to the new FC bridge. 
 Set the IP address of the new FC bridge.  

The LTO tape drive module in the PV136T LTO Library is secured to the chassis with:

   A drive filler plate. 
 One thumbscrew. 
 A handle. 
 Two thumbscrews. **

Choose all that Apply 
Before removing the Y-Axis flex cable, the following FRUs must be first removed from the PV136T LTO Library:

   Power distribution PCBA. *
 AC input module. *
 Display panel assembly. 
 Picker Assembly. *

