Servers - Dell RAID Controllers Product Certification Version 4.0

There are 24 questions, you have 100 minutes.

Multiple choice:
The PERC 2/Si is embedded in the following Dell server:
PE2400.
PE6450.
PE2450.
PE4400.

True/False:
The PERC 2 RAID Controller contains six separate channels - four external and two internal.
False.
True.

True/False:
The PERC 2 contains four channels and six SCSI connectors.
False.
True.

Mutliple choice:
What type of memory module is installed in the PERC 2/DC?
RIMM.
SIMM.
DIMM.
ECC.

True/False:
The firmware on the PERC 2 card must be updated to level 2.1 if the FAST utility used with it is version 2.1.
True.
False.

Choose all that apply:
The Perc 2/DC contains the following features:
Two internal SCSI connectors.
A cache battery.
Four external SCSI connectors.
Two channels.

Multiple choice:
Where is the PERC 3/Di cache battery located?
On top of the options bay in the PE4400.
On the PE2450 system board.
With the PE4400 system board battery.
On the PE4400 system board.

True/False:
The PowerEdge 6450 supports embedded RAID.
True.
False.

Choose all that apply:
The PERC 2/SC contains the following features:
One SCSI channel.
One internal SCSI connector.
One external SCSI connector.
A cache battery.

True/False:
SCSI cables can be attached to the PERC 2/SC for both external and internal hard-disk drives at the same time.
True.
False.

True/False:
SCSI cables can be attached to the PERC 2/DC for both internal and external hard-disk drives at the same time.
False.
True.

Multiple choice:
The PERC 2/Si RAID controller key is inserted into:
The RAID controller card.
The DRAC2 card.
The system board.
PCI slot two.

Multiple choice:
The PERC 3/Si cache memory is inserted into:
PCI slot three.
The system board.
Server system memory slot four.
The RAID controller card.

Choose all that apply:
Which of the following must be removed before removing the PERC 3/Di cache memory battery?
CD-ROM Drive.
The PE4400 processor cover.
PERC 3/Di cache memory module.
The PE4400 side cover.

True/False:
New hard-disk drives must be initialized first before creating a container on the PERC 3/Si RAID Controller when using the Adaptec BIOS configuration utility.
True.
False.

True/False:
The PERC 2 RAID Controller BIOS configuration utility is entered by pressing Ctrl M.
False.
True.

True/False:
The PERC 2 RAID Controller BIOS configuration utility is entered by pressing Ctrl M.
False.
True.

True/False:
The PERC 3/Si RAID controller alarm is silenced by selecting adapter, alarm, silence.
True.
False.

Multiple Choice:
What is the most efficient and default chunk size to use when setting up a RAID 5 on a PERC 3/Di RAID Controller?
128 KB.
32 MB.
64 KB.
32 KB.

True/False:
A scrub operation destroys data on the hard-disk drives when using a PERC 3/Si RAID controller.
True.
False.

Choose all that apply:
The following operations are performed while Configuring a RAID array on a Dell PERC 2/SC RAID controller:
Initialize an array.
Initialize a container.
Scrub.
Enable the alarm.

Multiple Choice:
The PERC 3/Di BIOS configuration utility is entered by pressing:
Ctrl Z
Alt A
Ctrl M
Ctrl A

Choose all that apply:
The RAID configuration for a PERC 2/DC RAID Controller is stored:
In system memory.
On the hard-disk drives in the array.
On the DOSA CD-ROM.
In NVRAM on the PERC 2/DC.

True/False:
When removing the PERC 2 RAID controller, the cache memory module must also be removed from the system board.
False.
True.