Servers – PowerEdge 1750 Product Certification

There are 15 questions, you have 60 minutes.

Multiple choice:
What must be replaced if an Unsupported CPU stepping detect error message is displayed on the PowerEdge1750?
System memory.
ERA/O.
CPU.
System board.

Multiple Choice:
What system setup option on the PowerEdge 1750 allows you to enable hyper-threading?
CPU information.
Boot sequence.
PCI IRQ assignment.
Integrated devices.

Multiple Choice:
What is the maximum amount of system memory the PowerEdge 1750 can support?
2 GB.
256 MB.
8 GB.
512 MB.

True/False:
The PowerEdge 1750 the riser board supports two 32-bit/33 MHz PCI cards.
False.
True.

Multiple Choice:
What is the maximum number of PCI cards that can be installed in the PowerEdge 1750?
Five.
Three.
Two.
Four.

Multiple Choice:
What RAID controller option is available on the PowerEdge 1750?
PERC 3/SI.
PERC 4/DI.
PERC 3/DCL.
PERC 3/DC.

Multiple Choice:
Where is the system status indicator for the cable management arm plugged into on the PowerEdge 1750?
Below the power supplies.
Behind the front bezel.
Below the expansion-card cage.
Next to the system identification button.

Multiple Choise:
On the PowerEdge 1750, the cable connecting the control panel to the system board is routed between which two components?
The floppy-diskette drive and the CD-ROM drive.
The front power supply and the ERA.
The front and back power supplies.
The front power supply and hard-disk drive 0.

Multiple Choice:
On the PowerEdge 1750, where is the metal tab located that is used to remove the CD-ROM?
Next to the system memory.
Next to the IDE CD-ROM cable.
Next to the system fan.
Under the control panel fan.

Choose all that apply:
What must be done before replacing the embedded remote administrator on the PowerEdge 1750?
Remove the front bezel.
Disconnect the ERA cable.
Remove the ROMB battery.
Open the top covers.

True/False:
On the PowerEdge 1750, you must press out on the memory module ejector on each end of the socket to remove a memory module.
False.
True.

Choose all that apply:
What must be done before removing the floppy diskette drive cable on the PowerEdge 1750?
Remove the front bezel.
Press the metal tab next to the front power supply. '
Open the top covers.
Pull the ZIF connector up.

Multiple Choice:
What must be done before removing the back power supply fan on the PowerEdge 1750?
Open the top covers.
Remove the front power supply.
Remove the back power supply.
Disconnect the back power supply fan cable.

Multiple Choice:
On the PowerEdge 1750, what must be removed before removing the PSDB?
PSDB shield.
VRM's.
System memory.
SCSI backplane.

Multiple Choice:
On the PowerEdge 1750, what secures the system board to the chassis?
A thumbscrew.
A solder joint.
A metal clamp.
Retaining clips.