Servers - PowerEdge 4600 Product Certification (25 Questions)

True/False:
The PowerEdge 4600 does not have to be removed from the rack before removing the front bezel.
True
False

Multiple Choice:
On the PowerEdge 4600, where are thumbscrews securing the system cover to the chassis located?
Next to the floppy-diskette drive.
Next to system board tray.
Next to the USB ports.
Next to the hard-disk drives.

Multiple Choice:
On the PowerEdge 4600, what must be removed first to replace a power supply?
The hard-disk drives.
The floppy-diskette drive.
The CD-ROM drive.
The front bezel.

Multiple Choice:
What must be removed before removing a SCSI hard-disk drive?
Serial cable.
Front bezel.
Drive-retention bracket.
Top system panels.

Multiple Choice:
On the PowerEdge 4600, what must be removed before removing a SCSI hard-disk drive?
SCSI backplane.
Front bezel.
CD-ROM.
Floppy-diskette drive.

Multiple Choice:
What is the maximum amount of RAM the PowerEdge 4600 will support?
8 GB.
6 GB.
12 GB.
14 GB.

Multiple Choice:
What is the maximum number of internal SCSI hard-disk drives the PowerEdge 4600 support?
Eight.
Six.
Ten.
Four.

Multiple Choice:
What is the embedded RAID option for the PowerEdge 4600 ?
PERC 2/SI.
PERC 3/DI.
PERC 3/SI.
PERC 2/DI.

Multiple Choice:
How many PCI slots does the PowerEdge 4600 contain?
Five.
Six.
Four.
Seven.

Multiple Choice:
What type of embedded controller is available for external devices?
Ultra3.
Ultra2.
IDE.
Narrow.

Multiple Choice:
What type of memory does the PowerEdge 4600 use?
SDRAM.
Rambus.
EDO.
DDR SDRAM.

True/False:
On the PowerEdge 4600, all system fans can be replaced individually.
True.
False.

Multiple Choice:
Where must the front fan assembly power cable be disconnected from?
System board.
CD-ROM.
SCSI backplane.
Media backplane assembly.

True/False:
A thumbscrew secures the peripheral bay assembly to the chassis.
True.
False.

Multiple Choice:
On the PowerEdge 4600, where is the floppy-diskette drive bracket assembly located?
Next to the system memory.
Next to the processors.
Next to the peripheral-bay assembly.
Next to the PCI slots.

Choose all that apply:
On the PowerEdge 4600, what must be done before removing the CD-ROM drive?
Remove the peripheral bay assembly.
Remove the system cover
Remove the floppy-diskette drive.
Remove the front bezel.

True/False:
You must push out on the peripheral-bay assembly retaining clips to remove the floppy-diskette drive.
False.
True.

Multiple Choice:
Where is the system board tray securing latch located?
On the front bezel.
Below the sytem board.
On the side of the system chassis.
Next to the SCSI backplane.

Choose all that apply:
What must be done before removing the fan shroud assembly?
Loosen the two thumbscrews.
Pull the SCSI cable up.
Remove the hot-plug PCI insulation.
Remove the power supplies.

Multiple Choice:
The PowerEdge 4600 contains how many memory card boards?
Two.
Six.
One.
Three.

Multiple Choice:
What is the bracket fan assembly attached to?
The system board.
The chassis.
The front bezel.
The peripheral bay assembly.

Multiple Choice:
Where is the ROMB battery backup located?
Next to the PSDB.
In the floppy-diskette drive bracket assembly.
Attached to the system cover.
Next to the ROMB key.

True/False:
The processor VRM's are soldered to the system board.
True.
False.

Choose all that apply:
What components must be transferred from the system board being replaced to the new system board when replacing a system board?
System memory.
VRMs.
Processors.
Power supplies.

On the PowerEdge 4600, how many processor retaining clips secure one processor to the system board?
Two.
One.
Three.
Four.