When a new version of IT Assistant is installed over an older one, the installation program saves the current IT Assistant database. 

   False  
 True  *

Which of the following can be selected when installing Management Station Applications? 

   Array Manager  *
 Remote Management  
 TCO Database Server 
 IT Assistant  *

When Array Manager is loaded on a system running Windows 2000 Server, what happens to the native disk management utility? 

   It is replaced by Array Manager.  *
 The native utility operates in the backgroud.  
 The native uutilities functionality is combined with Array Manager.  
 Nothing, both can be used.  

Which keys must be pressed to access the PERC 2, 2/Si, 3/Si or 3/Di BIOS configuration utility? 

   <Alt> <A> 
 <Ctrl> <A>  *
 <Ctrl> <M>  
 <Ctrl> <H>  

Which of the following firmware interfaces are available on the PERC 3/DCL, PERC, 3/DC, and PERC 3/QC? 

   Ctrl-H: WebBIOS Utility  *
 Ctrl-M: Adapter BIOS Utility * 
 Ctrl-G: GUI BIOS Utility  
 Ctrl-Q: Quick Setup Utility  

To install IT Assistant, must select the Install Management Station button when prompted to select the system type. 

   False  
 True  *

Array Manager supports AMI/LSI and Adaptec based PERCs. 

   True  *
 False  

What operating systems can IT Assistant be installed on? 

   Novell Netware 
 Windows XP  * (Not sure - One of the mail compot)
 Windows 2000 Professional  *
 Red Hat Linux  

What RAID level does NOT provide fault tolerance? 

   RAID 1  
 RAID 5  
 RAID 0  *
 RAID 3  

The acronym RAID stands for: 

   Reliable Array of Inexpensive Drives  
 Redundant Array of Interconnected Disks  
 Redundant Array of Independent Disks  *
 Reliable Array of Inexpensive Disks  

Multiple chioce: What is the purpose of expanding a virtual disk using Dell OpenManage Array Manager? 

   To decrease the size of an existing array.  
 To change disk type.  
 To add a disk to an existing array.  *
 To recover from a failed drive.  

The Diagnostic Service is installed by default when installing Server Administrator. 

   False 
 True  *

What management protocol must be installed and configured prior to installing Server Administrator? 

   DHCP  
 SNMP  *
 RIP  
 SMTP  

Dell OpenManage Array Manager manages storage resources on remote stations with the following operating system: 

   Netware 5.0  
 Windows 98  
 Windows 2000 Advanced Server *
 NT 4.0 Server  *

What must be specified when creating a virtual disk using Dell OpenManage Array Manager? 

   Set the permissions for the virtual disk to read only  
 The virtual disk size  
 Disk name  
 Format type  

With the PASSWD jumper installed on a PowerEdge 400SC, the password feature is disabled. 

   True  
 False *

The PowerEdge 400SC has an embedded Gigabit Ethernet NIC. 

   True  *
 False 

What is the cause of a 3-4-2 beep code error that occurs during a PowerEdge 400SC system startup? 

   DMA initialization failure  
 Time of day-clock stopped  
 Screen-retrace test failure or test in progress  *
 System configuration check failure  

The PowerEdge 1750 has ________ embedded Broadcom NetXtreme Gigabit NICs. 

   One 
 Three  
 Zero  
 Two  *
What must be replaced if an Unsupported CPU stepping detect error message is displayed on the PowerEdge1750? 

   CPU  *
 System board  
 ERA/O 
 System memory  

What must be replaced if the Time of Day clock fails on the PowerEdge 650? 

   System board coin battery  *
 Backplane  
 Power supply  
 DIMMs  

On the PowerEdge 650, the default position of the NVRAM_CLR jumper is set to enabled (jumpered). 

   False  *
 True  

When replacing an EMM on the powerVault 220S or PowerVault 221S, what can be done to ensure data is not lost due to improper termination? 

   Remove all the split-bus modules.  
 Quickly insert a terminator module into the empty slot.  
 Switch the enclosure into cluster mode.  
 Power down the enclosure. *

On the PowerVault 220S and PowerVault 221S the ______ LED will be on when the backplane is split into two separate SCSI buses. 

   Cluster 
 Power  
 Fault  
 Split-bus  *

What option must be installed to support eight hard-disk drives internally on the PowerEdge 2600? 

   Split backplane card  
 Peripheral bay backplane  *
 ROMB hardware  
 1 x 8 SCSI backplane  

What type of memory does the PowerEdge 4600 use? 

   EDO  
 Rambus  
 SDRAM  
 DDR SDRAM  *

On the PowerEdge 6600, you can only remove and replace one power supply at a time when the system is powered on. 

   False 
 True  *

What command would test basic connectivity of a PowerConnect 5224 switch? 

   nbtstat 
 path 
 ping *
 ipconfig 

The PowerConnect 5212 has 24 one gigabit Ethernet port. 

   False *
 True 
 
What components are field replaceable on the PowerConnect 5212? 

   Fan pack  
 SFP *
 Network Switch * (This means the whole switch, but not sure) 
 Power Supply 


90% Good Luck!!


 






 



 







