Question # 1 of 30

You have 120 minutes left (as of the time this page was requested from the server).

Multiple Choice
What tool is required when replacing a PowerConnect 5224 mounted in a Dell rack?

   5/8' Open Ended Wrench 
 T-20 Torx Driver 
 #2 Phillips-Head Screwdriver ***
 Flathead Screwdriver 


Question # 2 of 30

You have 106 minutes left (as of the time this page was requested from the server).

Multiple Choice
What type of serial cable must be used when connecting to the PowerConnect 3248? 

   Null Modem serial cable
 USB cable 
 Firewire cable 
 Straight-through serial cable  ***

Question # 3 of 30

You have 100 minutes left (as of the time this page was requested from the server).

Multiple Choice
What command would test basic connectivity of a PowerConnect 5224 switch? 

   path 
 ipconfig 
 ping ***
 nbtstat 

Question # 4 of 30

You have 95 minutes left (as of the time this page was requested from the server).

True/False:
On the PowerEdge 6600, you can only remove and replace one power supply at a time when the system is powered on. 

   False 
 True  ***

Question # 5 of 30

You have 91 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What type of memory does the PowerEdge 4600 use? 

   SDRAM  
 EDO  
 DDR SDRAM  ***
 Rambus  


Question # 6 of 30

You have 87 minutes left (as of the time this page was requested from the server).

True/False:
The PowerEdge 2600 contains an RJ45 connector that can be used for the embedded remote access card option. 

   False  
 True  ***

Question # 7 of 30

You have 85 minutes left (as of the time this page was requested from the server).

True/False:
The Enclosure Management Modules on the PowerVault 220S and PowerVault 221S are hot-swappable. 

   False ***
 True  



Question # 8 of 30

You have 82 minutes left (as of the time this page was requested from the server).

Choose all that apply:
A PowerVault 220S and a PowerVault 221S have indicator LEDs on which of the following modules? 

   The front panel  ***
 The enclosure management module  ***
 The active cooling module *
 Split-bus module  ***

What is the embedded RAID option on a PowerEdge 4600? 

   PERC 2/DI  
 PERC 2/SI  
 PERC 3/DI ***
 PERC 3/SI  

When a new version of IT Assistant is installed over an older one, the installation program saves the current IT Assistant database. 

   True  ***
 False  


Question # 9 of 30

You have 78 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What feature allows clearing of the system password in the event the system password is forgotten or becomes corrupted on the PowerEdge 650? 

   System security option in the system BIOS  
 Removing the coin battery on the systemboard * 
 Pressing the power button three times  
 The password jumper on the system board (Answer)??? 



Question # 10 of 30

You have 74 minutes left (as of the time this page was requested from the server).

Multiple Choice:
A blue blinking system status indicator on the PowerEdge 650 indicates? 

   There is activity on the NIC  
 The power is off  
 The system is identifying itself  ***
 A fault with the hard-disk drive  


Question # 11 of 30

You have 73 minutes left (as of the time this page was requested from the server).

Multiple Choice:
The PowerEdge 1750 has ________ embedded Broadcom NetXtreme Gigabit NICs. 

   Three  
 One 
 Two  *
 Zero  


Question # 12 of 30

You have 72 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What does a 4-3-1 beep code indicate on the PowerEdge 1750? 

   Improperly installed, or faulty memory modules  ***
 Cache test failure, or faulty microprocessor  
 No memory installed  
 Faulty mouse cable  


Question # 13 of 30

You have 71 minutes left (as of the time this page was requested from the server).

Multiple Choice:
How many external USB ports are supported on the PowerEdge 400SC? 

   One  
 Six ***
 Four  
 Five  


Question # 14 of 30

You have 69 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What is the maximum number of PCI cards that can be installed in a PowerEdge 400SC? 

   Three  
 Two  
 Four  ***
 Five 


Question # 15 of 30

You have 68 minutes left (as of the time this page was requested from the server).

Multiple Choice:
On a PowerEdge 400SC, what is the possible problem when the rear panel LED indicators are lit as follows: A=Red, B=Green, C=Red, D=Red? 

   PCI device configuration activity in progress or PCI device failure.  ***
 Loose connection on your printer.  
 Loose or improperly connected mouse. 
 Ethernet cable connected in wrong port.  


Question # 16 of 30

You have 66 minutes left (as of the time this page was requested from the server).

Choose all that apply:
What must be specified when creating a virtual disk using Dell OpenManage Array Manager? 

   Format type  *
 Set the permissions for the virtual disk to read only  
 Disk name  *
 The virtual disk size  *



Question # 17 of 30

You have 65 minutes left (as of the time this page was requested from the server).

True/False:
The Diagnostic Service is installed by default when installing Server Administrator. 

   True*  
 False 


Question # 18 of 30

You have 64 minutes left (as of the time this page was requested from the server).

True/False:
The SNMP community name cannot be specified during a Windows 2000 installation when using the Dell OpenManage Server Assistant CD. 

   True  ***
 False  


Exam # 467 : Associate Server Certification V6.0

Question # 19 of 30

You have 58 minutes left (as of the time this page was requested from the server).

Choose all that apply:
What utilities are contained in the utility partition created using the Dell OpenManage Server Assistant CD? 

   Server Diagnostics  *
 BIOS Update Utility  *
 RAID Utility  *
 Server Administrator 


Question # 20 of 30

You have 57 minutes left (as of the time this page was requested from the server).

Multiple chioce: What is the purpose of expanding a virtual disk using Dell OpenManage Array Manager? 

   To change disk type.  
 To add a disk to an existing array.  ***
 To recover from a failed drive.  
 To decrease the size of an existing array.  


Question # 21 of 30

You have 57 minutes left (as of the time this page was requested from the server).

True/False:
System storage can be set up using the Dell OpenManage Array Manager Tool from the Dell OpenManage Server Assistant CD. 

   False  
 True  *


Question # 22 of 30

You have 54 minutes left (as of the time this page was requested from the server).

Multiple Choice:
The acronym RAID stands for: 

   Redundant Array of Interconnected Disks  
 Reliable Array of Inexpensive Disks  
 Redundant Array of Independent Disks  ***
 Reliable Array of Inexpensive Drives  



Question # 23 of 30

You have 54 minutes left (as of the time this page was requested from the server).

Choose all that apply:
What operating systems can IT Assistant be installed on? 

   Windows XP  ***
 Red Hat Linux  
 Windows 2000 Professional  ***
 Novell Netware 


Question # 24 of 30

You have 52 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What management protocol must be installed and configured prior to installing Server Administrator? 

   SMTP  
 DHCP  
 RIP  
 SNMP  ***



Question # 25 of 30

You have 51 minutes left (as of the time this page was requested from the server).

Choose all that apply:
What functions can be performed from the Quick Access menu in Dell OpenManage Array Manager? 

   Remote Management  ***
 Create a volume  ***
 Run Diagnostics  
 Set policies  



Question # 26 of 30

You have 50 minutes left (as of the time this page was requested from the server).

Choose all that apply:
Dell OpenManage Array Manager manages storage resources on remote stations with the following operating system: 

   Windows 2000 Advanced Server *
 NT 4.0 Server  *
 Windows 98  
 Netware 5.0  


Question # 27 of 30

You have 45 minutes left (as of the time this page was requested from the server).

Multiple Choice:
When Array Manager is loaded on a system running Windows 2000 Server, what happens to the native disk management utility? 

   The native utility operates in the backgroud.  
 It is replaced by Array Manager.  *
 The native uutilities functionality is combined with Array Manager.  
 Nothing, both can be used.  


Question # 28 of 30

You have 43 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What Server Administrator tab allows you to view the POST logs? 

   Shutdown  
 Properties  
 Diagnostics  
 Logs  ***


Question # 29 of 30

You have 43 minutes left (as of the time this page was requested from the server).

True/False:
To install Server Administrator, you will need to select the Install Management "Station"??? button when prompted for Select System Type. 

   True  *?????
 False  


Question # 30 of 30

You have 40 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What RAID level does NOT provide fault tolerance? 

   RAID 5  
 RAID 3  
 RAID 0  ***
 RAID 1  


70%


What components are field replaceable on the PowerConnect 5212? 

   SFP *
 Network Switch 
 Power Supply 
 Fan pack  

Question # 2 of 30

You have 117 minutes left (as of the time this page was requested from the server).

True/False
Network devices can communicate through a PowerConnect 3248, whether the Ethernet cable is straight-through or crossover. 

   False ???
 True 

Question # 3 of 30

You have 115 minutes left (as of the time this page was requested from the server).

Choose all that Apply
What two files can the customer upgrade without support intervention on a PowerConnect 5212? 

   loader file  
 config file ***
 diag file  
 opcode file ***

Question # 4 of 30

You have 112 minutes left (as of the time this page was requested from the server).

True/False:
If neither the split-bus LED nor the cluster LED are illuminated, the enclosure is in cluster mode. 

   True  
 False ***

Question # 5 of 30

You have 112 minutes left (as of the time this page was requested from the server).

Multiple Choice:
On the PowerEdge 6600, what is the minimum number of power supplies required for the operating system to operate normally? 

   One  
 Four  
 Three  
 Two ***

Question # 6 of 30

You have 110 minutes left (as of the time this page was requested from the server).

True/False:
The processor VRMs on the PowerEdge 4600 are soldered to the system board. 

   True  
 False  ***


Question # 9 of 30

You have 106 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What are the minimum and maximum amounts of memory that can be installed in a PowerEdge 400SC? 

   512 MB – 2 GB  
 256 MB – 4 GB  
 128 MB – 4 GB  ***
 128 MB – 2 GB  


Question # 11 of 30

You have 101 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What is the minimum and maximum amount of memory that can be supported by the PowerEdge 650? 

   1 GB/8 GB  
 128 MB/4 GB  ***
 512 K/2 GB  
 256 MB/1 GB  


Question # 12 of 30

You have 100 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What is the maximum number of processors that can be installed in the PowerEdge 650? 

   Four  
 Three 
 Two  
 One  ***

Question # 13 of 30

You have 100 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What system setup option on the PowerEdge 1750 allows you to set the maximum memory available to the operating system to 256 MB? 

   Integrated devices 
 OS install mode  ***
 Embedded server management  
 PCI IRQ assignment  


Question # 18 of 30

You have 92 minutes left (as of the time this page was requested from the server).

True/False:
System storage can be set up using the Dell OpenManage Array Manager Tool from the Dell OpenManage Server Assistant CD. 

   True  ***
 False  

True/False
When using Telnet, changes made to the running configuration will automatically be saved to the startup configuration on a PowerConnect 3248. 

   True 
 False ***


Multiple Choice:
What is the maximum number of Xeon microprocessors that a PowerEdge 6600 or 6650 will support? 

   Two  
 One  
 Four ***
 Three  


Multiple Choice:
What option must be installed to support eight hard-disk drives internally on the PowerEdge 2600? 

   Peripheral bay backplane  
 ROMB hardware  
 1 x 8 SCSI backplane*  
 Split backplane card 

The PowerVault 220S and the PowerVault 221S support up to 12 1-inch Ultra-3 SCSI hard-disk drives. 
Flase***

A PowerVault 220S or PowerVault 221S in a non-redundant configuration will have a _____ installed in the secondary EMM slot. 

   RAID controller  
 SCSI Terminator card  ***
 Filler panel  
 Split-bus module 

What must be replaced if the Time of Day clock fails on the PowerEdge 650? 

   DIMMs  
 System board coin battery  *???
 Power supply  
 Backplane  

 What must be replaced if an Unsupported CPU stepping detect error message is displayed on the PowerEdge1750? 

   ERA/O 
 CPU  ***
 System memory  
 System board  

What is the cause of a 3-4-2 beep code error that occurs during a PowerEdge 400SC system startup? 

   Time of day-clock stopped  
 Screen-retrace test failure or test in progress  ***
 DMA initialization failure  
 System configuration check failure  

Which keys must be pressed to access the PERC 2, 2/Si, 3/Si or 3/Di BIOS configuration utility? 

   <Ctrl> <A>  ***
 <Ctrl> <H>  
 <Ctrl> <M>  
 <Alt> <A> 

The PowerConnect 5212 has 24 one gigabit Ethernet port. 

   True 
 False ***

On a PowerConnect 3248, which command would set a port to 10 Mb full duplex at the 'Console(config-if)#' prompt? 

   speed 10full *** 
 speed-duplex 100half  
 speed-duplex 10full 
 speed-fullduplex 10mb  

When replacing an EMM on the powerVault 220S or PowerVault 221S, what can be done to ensure data is not lost due to improper termination? 

   Remove all the split-bus modules.  
 Switch the enclosure into cluster mode.  
 Power down the enclosure.  ***
 Quickly insert a terminator module into the empty slot.  

What is the processor frontside bus speed on the PowerEdge 650? 

   200 MHz ***
 133 MHz  
 533 MHz  
 100 MHz  

How many processors will the PowerEdge 1750 support? 

   Four  
 Two  ***
 One  
 Three 

To install Server Administrator, you will need to select the Install Management Station button when prompted for Select System Type. 

   True  
 False  **

Which of the following firmware interfaces are available on the PERC 3/DCL, PERC, 3/DC, and PERC 3/QC? 

   Ctrl-H: WebBIOS Utility  ***
 Ctrl-Q: Quick Setup Utility  
 Ctrl-G: GUI BIOS Utility  
 Ctrl-M: Adapter BIOS Utility  ***

Which of the following can be selected when installing Management Station Applications? 

   IT Assistant  **
 TCO Database Server 
 Array Manager  **
 Remote Management  

True/False:
To install IT Assistant, must select the Install Management Station button when prompted to select the system type. 

   False  
 True  ***

Array Manager supports AMI/LSI and Adaptec based PERCs. 

   False  
 True  ***

