# Storage – PowerVault 122T Autoloader Product Certification

There are 10 questions, you have 40 minutes.

Multiple Choice
The buttons on the front button operator panel of the PV122T provide access to the following information:
System BIOS level.
System service tag number.
Diagnostics.
Tape speed.

Choose all that apply
The following LED indicators present drive status of the PV122T:
Ready/Activity.
Error.
Tape Loaded.
Clean Drive.

True/False
The PV122T autoloader contains space to store nine tape cartridges.
True.
False.

Multiple choice
The native capacity of the PV122T is:
240 GB.
280 GB.
640 GB.
320 GB.

Multiple Choice
Cables are held in place on the back of the PV122T with:
A cable-routing bracket.
Cable channels.
Two thumb-screws.
Cable ties.

Multiple Choice
The PV122T is secured to the rack with the following:
Slide rails.
Two thumb-screws on the ears.
Phillips-head screws.
A clamp.

True/False
The PV122T can be installed in a rack using rapid rails or VersaRails.
False.
True.

True/False
The PV122T can be installed in a rack using rapid rails or VersaRails.
False.
True.

Choose All that apply
Remove the following components first before removing the stuck tape from a PV122T:
Rail ears and screws.
System fan.
Left receiver.
Top cover.

Choose all that apply
The following components must be removed completely from the PV122T when removing a stuck tape cartridge:
LED/eject button bracket.
Right receiver.
Power supply.
Left receiver.