Servers - PERC 3 DCL/DC/QC Product Certification (10 Questions)

Choose all that apply:
Which of the following RAID controllers offer 128 MB of transportable battery-backed cache?
None of these selections.
PERC 3/QC.
PERC 3/DCL.
PERC 3/DC.

Choose all that apply:
Which of the following RAID levels are supported on the PERC 3/DCL, PERC 3/DC, and PERC 3/QC?
RAID "10"
RAID 5.
RAID 1.
RAID 3.

Multiple choice:
Which of the following describes the PCI interface on the PERC 3/DCL, PERC 3/DC, and PERC 3/QC?
32-bit, 33 MHz PCI 2.1.
64-bit, 66 MHz PCI 2.2 (not compatible with 32-bit or 33 MHz PCI slots).
MiniPCI.
64-bit, 66 MHz PCI 2.2 (compatible with 32-bit and 33 MHz PCI slots).

Choose all that apply:
Which of the following firmware interfaces are available on the PERC 3/DCL, PERC 3/DC, and PERC 3/QC?
Ctrl-H: WebBIOS Utility.
Ctrl-M: Adapter BIOS Utility.
Ctrl-Q: Quick Setup Utility.
Ctrl-G: GUI BIOS Utility.

Multiple choice:
Which of the following tasks should be completed when migrating cache from a failed PERC 3/DC or PERC 3/QC to a replacement?
Pay attention to which cable is connected to which SCSI channel on the original controller and match the cabling on the replacement controller.
None of these selections are correct.
Connect a SCSI cable between the two adapters to transfer the cache data.
Disconnect the battery before removing the cache.

True/False:
The PERC 3/DC and PERC 3/QC can retain unwritten cache data for up to 72 hours.
False.
True.

True/False:
When using Dell OpenManage Array Manager to configure a virtual disk on the PERC 3/DCL, PERC 3/DC, or PERC 3/QC; if drives of multiple capacities are mixed in a single virtual disk, all drives are truncated to the size of the smallest member.
False.
True.

Multiple choice:
Which of the following do you right-click to begin creating a virtual disk in Dell OpenManage Array Manager?
Physical Array under Arrays - PERC Subsystem.
The Disks folder.
The DM View tab.
Array Group 0 under Arrays - PERC Subsystem - Logical Array.

Multiple choice:
What must you do before you can use Dell OpenManage Array Manager to create a volume on a new virtual disk controlled by the PERC 3/DCL, PERC 3/DC, or PERC 3/QC?
Locate the unsigned disk that corresponds to the new virtual disk, and write a signature to it.
Shut down and restart the Dell PowerEdge server.
No additional steps are necessary, the virtual disk is automatically prepared for use by the operating system.
Click the -Prepare Virtual Disk- button.

Multiple choice:
What must you right-click in Dell OpenManage Array Manager to configure a global hot spare for virtual disks on a PERC 3/DCL, PERC 3/DC, or PERC 3/QC?
The Volumes folder.
Any Array Disk under Array - PERC Subsystem - Logical Array - Array Group 0.
Any unassigned Array Disk under Array - PERC Subsystem - Logical Array - Array Group 0.
Physical Array under Array - PERC Subsystem.