Question # 1 of 30

You have 120 minutes left (as of the time this page was requested from the server).

Choose all that Apply
What components are field replaceable on the PowerConnect 5212? 

Network Switch 		*
SFP 			*
Power Supply 
Fan pack  




Question # 2 of 30

You have 118 minutes left (as of the time this page was requested from the server).

Multiple Choice
What is the default username and password, to manage the PowerConnect 3248 in Privileged Exec mode?

'administrator', blank password 
'admin','admin'  		*
'admin', 'password' 
'user','privilege' 



Question # 3 of 30

You have 118 minutes left (as of the time this page was requested from the server).

Multiple Choice
What command saves the PowerConnect 5212 switch's running configuration to the startup configuration? 

move running-conf startup-conf  
copy running-config startup-config  *
save running-cfg startup-cfg  
copy start-cfg running-cfg  


Question # 4 of 30

You have 118 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What is the maximum number of Xeon microprocessors that a PowerEdge 6600 or 6650 will support? 

Two  
One  
Four  *
Three  



Question # 5 of 30

You have 117 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What type of memory does the PowerEdge 4600 use? 

Rambus  
DDR SDRAM  *
EDO  
SDRAM




Question # 6 of 30

You have 117 minutes left (as of the time this page was requested from the server).

True/False:
The PowerEdge 2600 contains an RJ45 connector that can be used for the embedded remote access card option. 

False  
True  *



Question # 7 of 30

You have 116 minutes left (as of the time this page was requested from the server).

Choose all that apply:
A PowerVault 220S and a PowerVault 221S have indicator LEDs on which of the following modules? 

   The active cooling module 		*
 Split-bus module  			*
 The front panel  			*
 The enclosure management module  	*



Question # 8 of 30

You have 112 minutes left (as of the time this page was requested from the server).

True/False:
The Enclosure Management Modules on the PowerVault 220S and PowerVault 221S are hot-swappable. 

   False *
 True  



Question # 9 of 30

You have 111 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What must be replaced if the Time of Day clock fails on the PowerEdge 650? 

DIMMs  
Backplane  
Power supply  
System board coin battery  *




Question # 10 of 30

You have 105 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What is the maximum number of processors that can be installed in the PowerEdge 650? 

Four  
Three 
Two  
One     *


Question # 11 of 30

You have 105 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What must be replaced if an Unsupported CPU stepping detect error message is displayed on the PowerEdge1750? 

System board  
CPU    *
ERA/O 
System memory  



Question # 12 of 30

You have 104 minutes left (as of the time this page was requested from the server).

Multiple Choice:
The PowerEdge 1750 has ________ embedded Broadcom NetXtreme Gigabit NICs. 

Zero  
One 
Two  *
Three 



Question # 13 of 30

You have 103 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What is the maximum number of PCI cards that can be installed in a PowerEdge 400SC? 

Five 
Three  
Four  *
Two  


Question # 14 of 30

You have 102 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What is the maximum number of processor(s) that can be installed in a PowerEdge 400SC? 

Two  
Four  
Three 
One  *



Question # 15 of 30

You have 101 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What are the minimum and maximum amounts of memory that can be installed in a PowerEdge 400SC? 

128 MB – 4 GB  *
128 MB – 2 GB  
512 MB – 2 GB  
256 MB – 4 GB  




Question # 16 of 30

You have 100 minutes left (as of the time this page was requested from the server).

Choose all that apply:
What must be specified when creating a virtual disk using Dell OpenManage Array Manager? 

The virtual disk size  						*
Set the permissions for the virtual disk to read only  
Format type  							*
Disk name  							*




Question # 17 of 30

You have 99 minutes left (as of the time this page was requested from the server).

True/False:
Array Manager supports AMI/LSI and Adaptec based PERCs. 

True     *
False  




Question # 18 of 30

You have 98 minutes left (as of the time this page was requested from the server).

Choose all that apply:
Which of the following firmware interfaces are available on the PERC 3/DCL, PERC, 3/DC, and PERC 3/QC? 

Ctrl-Q: Quick Setup Utility  
Ctrl-M: Adapter BIOS Utility    *
Ctrl-G: GUI BIOS Utility  
Ctrl-H: WebBIOS Utility  	 *




Question # 19 of 30

You have 98 minutes left (as of the time this page was requested from the server).

Choose all that apply:
What operating systems can IT Assistant be installed on? 

Windows 2000 Professional  *
Novell Netware 
Red Hat Linux  
Windows XP  		      *



Question # 20 of 30

You have 96 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What management protocol must be installed and configured prior to installing Server Administrator? 

SNMP    *
DHCP  
RIP  
SMTP  




Question # 21 of 30

You have 95 minutes left (as of the time this page was requested from the server).

Choose all that apply:
Which of the following can be selected when installing Management Station Applications? 

IT Assistant  		*
TCO Database Server 
Remote Management  
Array Manager  		*







Question # 22 of 30

You have 95 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What Server Administrator tab allows you to view the POST logs? 

Shutdown  
Diagnostics  
Logs  		*
Properties  
	



Question # 23 of 30

You have 89 minutes left (as of the time this page was requested from the server).

Choose all that apply:
What utilities are contained in the utility partition created using the Dell OpenManage Server Assistant CD? 

Server Diagnostics  *
BIOS Update Utility   *
RAID Utility  	       *	
Server Administrator 






Question # 24 of 30

You have 88 minutes left (as of the time this page was requested from the server).

Multiple Choice:
The acronym RAID stands for: 

Reliable Array of Inexpensive Disks  
Reliable Array of Inexpensive Drives  
Redundant Array of Independent Disks     *
Redundant Array of Interconnected Disks  




Question # 25 of 30

You have 88 minutes left (as of the time this page was requested from the server).

Multiple Choice:
Which keys must be pressed to access the PERC 2, 2/Si, 3/Si or 3/Di BIOS configuration utility? 

<Ctrl> <H>  
<Ctrl> <A>      *
<Alt> <A> 
<Ctrl> <M>




Question # 26 of 30

You have 87 minutes left (as of the time this page was requested from the server).

True/False:
When a new version of IT Assistant is installed over an older one, the installation program saves the current IT Assistant database. 

False  
True    *



Question # 27 of 30

You have 86 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What RAID level does NOT provide fault tolerance? 

RAID 3  
RAID 1  
RAID 5  
RAID 0    *



Question # 28 of 30

You have 86 minutes left (as of the time this page was requested from the server).

Choose all that apply:
What functions can be performed from the Quick Access menu in Dell OpenManage Array Manager? 

Set policies  
Create a volume 	*	 
Remote Management  	*
Run Diagnostics  




Question # 29 of 30

You have 86 minutes left (as of the time this page was requested from the server).

True/False:
The Diagnostic Service is installed by default when installing Server Administrator. 

True  
False   *




Question # 30 of 30

You have 83 minutes left (as of the time this page was requested from the server).

Multiple chioce: What is the purpose of expanding a virtual disk using Dell OpenManage Array Manager? 

To change disk type.  
To add a disk to an existing array.   *
To recover from a failed drive.  
To decrease the size of an existing array 






  









 






 




  



