Servers PowerEdge 1650

Multiple Choice:
Where is the top system panel lock release located on the PowerEdge 1650?
Next to the CD-ROM.
Next to the back PCI slots.
Next to the back USB connections.
Next to the front USB connection.

True/False:
The PowerEdge 1650 must be removed from the rack before removing the front bezel.
True.
False.

Multiple Choice:
What channel are the IDE hard-disk drives connected to on the PowerEdge 1650?
Primary IDE channel.
Secondary SCSI channel.
Secondary IDE channel.
Primary SCSI channel.

Multiple Choice:
On the PowerEdge 1650, how many hard-disk drives are hot swappable when connected to the onboard Adaptec 7899 SCSI controller?
Two.
One.
Three.
None.

Multiple Choice:
What must be removed before removing a SCSI hard-disk drive?
Drive-retention bracket.
Top system panels.
Front bezel.
Serial cable.

True/False:
A PowerEdge 1650 configured with IDE hard-disk drives will not contain a hard-disk drive backplane.
False.
True.

Multiple Choice:
Where is the metal tab located that is used to remove the CD-ROM on the PowerEdge 1650?
Next to the system fan.
Under the control panel fan.
Next to the system memory.
Next to the IDE CD-ROM cable.

Choose all that apply:
What must be done before removing the floppy-diskette drive cable on the PowerEdge 1650?
Open the top panels.
Remove the front bezel.
Pull the ZIF connector up.
Press the metal tab next to the front power supply.

True/False:
To replace the back power supply on the PowerEdge 1650, slide the back power supply towards the front of the system.
False.
True.

Multiple Choice:
What must be done before removing the back power supply fan on the PowerEdge 1650?
Remove the front power supply.
Remove the back power supply.
Disconnect the back power supply fan cable.
Remove the PSDB.

Multiple Choice:
On the PowerEdge 1650, where is the fan bracket release located?
Next to the front power supply.
Next to the PCI riser board.
Next to the control panel.
Next to the CD-ROM drive.

Multiple Choice:
Where is the SCSI backplane board handle located on the PowerEdge 1650?
A SCSI backplane release tab does not exist.
Between the SCSI backplane and the CD-ROM drive.
Between the SCSI backplane and the VRM's.
Behind the floppy-diskette drive next to the SCSI backplane release latch.

True/False:
You must loosen the PCI expansion card latch in order to replace a PCI expansion card on the PowerEdge 1650.
True.
False.

Choose all that apply:
What must be done before replacing the PCI expansion riser board on the PowerEdge 1650?
Remove the front bezel.
Remove any PCI expansion cards.
Open the top panel.
Remove the system fans.

Multiple Choice:
What cable connection should be verified when replacing the ROMB mezzanine board on the PowerEdge 1650?
The SCSI cable.
The battery cable.
The ROMB cache connection cable.
The riser cable.

Multiple Choice:
On the PowerEdge 1650, what secures the system board to the chassis?
Retaining clips.
A metal clamp.
A thumbscrew.
A solder joint.

Multiple Choise:
On the PowerEdge 1650, the cable connecting the control panel to the system board is routed between what two components?
The front power supply and hard-disk drive 0.
The front and back power supplies.
The front power supply and the ERA.
The floppy-diskette drive and the CD-ROM drive.

Multiple Choice:
Where is the PSDB located on the PowerEdge 1650?
Built into the SCSI backplane.
Next to the PCI expansion riser board.
Between the floppy-diskette drive and CD-ROM drive.
Power supply bay area.

Multiple Choice:
On the PowerEdge 1650, what must be removed before removing the PSDB?
SCSI backplane.
System memory.
PSDB shield.
VRM's.

True/False:
On the PowerEdge 1650, you must press out on the memory module ejector on each end of the socket to remove a memory module.
True.
False.

True/False:
On the PowerEdge 1650, a terminator card is required if there is only one processor in installed in the system.
True.
False.

Multiple Choice:
To replace a processor on the PowerEdge 1650, which of the following components must be removed?
Processor heat sink.
VRM.
PSDB.
System memory.

Choose all that apply:
What must be done before replacing the embedded remote administrator card on the PowerEdge 1650?
Remove the front bezel.
Disconnect the ERA cable.
Disconnect the ERA network cable.
Open the top panels.

True/False:
The riser board supports two 32-bit/33 MHz PCI cards.
False.
True.

Multiple Choice:
What is the maximum amount of system memory the PowerEdge 1650 can support?
4 GB.
256 MB.
2 GB.
512 MB.

Multiple Choice:
How many processors will the PowerEdge 1650 support?
Three.
Two.
One.
Four.

True/False:
The CD-ROM device is connected to the secondary channel when IDE hard-disk drives are installed.
True.
False.

Multiple Choice:
What RAID option is available for the internal SCSI drives on the PowerEdge 1650?
PERC 3/SI.
PERC 3/DCL.
PERC 3/DI.
PERC 3/DC.

Multiple Choice:
The PowerEdge 1650 has ___ embedded Intel Pro 1000 XT Gigabit NICs.
Zero.
Three.
One.
Two.

Multiple Choice:
Which Adaptec SCSI controller is integrated into the system board on the PowerEdge 1650?
AIC-7890.
AIC-7799.
AIC-7899W.
AIC-7860.