Servers - PowerEdge 650 Product Certification

# There are 15 questions, you have 60 minutes

True/False
The PowerEdge 650 requires the system memory to be populated in pairs.
False.
True.

Multiple choice:
On the PowerEdge 650, what does a 'GATE A20 failure' message indicate?
Improperly installed memory module.
NVRAM_CLR jumper is installed.
Faulty keyboard controller.
Bad mouse cable.

Multiple choice:
The PowerEdge 650 has ________ DIMM sockets.
One.
Four.
Three.
Two.

True/False
The DRACIII/XT must be installed in the PCI-X (64 bit/133 MHz) slot of the riser board in the PowerEdge 650.
False.
True.

Multiple choice:
What feature allows clearing of the system password in the event the system password is forgotten or becomes corrupted on the PowerEdge 650?
Pressing the power button three times.
System security option in the system BIOS.
The password jumper on the systemboard.
Removing the coin battery on the systemboard

True/False
If the PowerEdge 650 locks with the NMI enabled in the system BIOS, pressing the NMI button will send an alert to the system.
True.
False.

Multiple choice:
What key(s) must be pressed on the PowerEdge 650 to enter into system setup during the POST?
F10.
F1.
Ctrl/Alt/Delete.
F2.

Multiple choice:
What key(s) must be pressed on the PowerEdge 650 to enter into system setup during the POST?
F10.
F1.
Ctrl/Alt/Delete.
F2.

True/False:
The front bezel must be removed from the PowerEdge 650 before removing the Backplane.
True.
False.

True/False
The chassis intrusion switch is located on the systemboard on the PowerEdge 650.
True.
False.

Multiple Choice:
Before removing the CD-ROM/floppy disk-drive on the PowerEdge 650, remove the following components:
The front bezel.
The system cover.
The power supply.
The hard-disk drives.

Multiple Choice:
Before removing the CD-ROM/floppy drive on the PowerEdge 650, do the following:
Remove the front bezel.
Remove the system from the rack.
Remove the removal storage bay unit.
Remove the system cover.

True/False
The CD-ROM\floppy diskette drive interposer board is held in place with Phillips-head screws.
True.
False.

Multiple choice:
The systemboard on the PowerEdge 650 is secured to the chassis using a:
Swivel hooks.
Thumbscrew.
Pop rivets.
Locking lever.

True/False:
On the PowerEdge 650 the CPU blower must be removed before removing the CPU.
True
False

Multiple choice:
On the PowerEdge 650, what does the system status indicator blinking blue indicate?
There is activity on the NIC.
A fault with the hard-disk drive.
The system is identifying itself.
The power is off.