Question # 1 of 38

You have 159 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What key must be pressed to access the utility partition during power on self test(POST)? 

   <F10> **
 <F8> 
 <F12> 

Question # 2 of 38

You have 158 minutes left (as of the time this page was requested from the server).

Multiple choice: 
What is a disadvantage of RAID 1? 

   It has poor fault tolerance compared to other RAID levels  
 It has poor single file I/O performance compared to other RAID levels 
 It has poor storage efficiency, requiring twice as many disk drives. (Answers)
 Performance is seriously reduced when a drive fails  **

Question # 3 of 38

You have 158 minutes left (as of the time this page was requested from the server).

Multiple choice: 
What is the purpose of the parity information stored in a RAID 3 array? 

   Provide rebuild data if a drive in the array fails.  ***
 Provide copies of data for simultaneous access by several applications.  
 Allow the RAID controller to test the validity of data stored.  
 Create a backup of files saved in the RAID array. 

Question # 4 of 38

You have 156 minutes left (as of the time this page was requested from the server).

Multiple choice: 
You should choose a RAID 10 configuration to combine the: 

   Fault tolerance of RAID 1 with the performance of RAID 0.  **
 Storage efficiency of RAID 1 with the fault tolerance of RAID 0.  
 Fault tolerance of RAID 5 with the performance of RAID 0.  
 Performance of RAID 5 with the fault tolerance of RAID 0. 

Question # 5 of 38

You have 156 minutes left (as of the time this page was requested from the server).

Multiple choice: 
What RAID level does NOT provide fault tolerance?

   RAID 3. 
 RAID 5. 
 RAID 0. **
 RAID 1. 

Question # 6 of 38

You have 155 minutes left (as of the time this page was requested from the server).

Multiple choice:
Which one of the following statements describes a feature of RAID 0? 

   It contains parity data. 
 It increases fault tolerance. 
 It provides 100% storage efficiency. **
 It creates a mirrored copy of data on a second disk. 

Question # 7 of 38

You have 154 minutes left (as of the time this page was requested from the server).

Multiple choice: 
Which of the following statements describes a stripe set? 

   The sizes of stripes in a stripe set are the same.  **
 A disk is reserved for all the stripes in a stripe set. 
 A stripe set stores a different file in each stripe. 
 The more disks there are in an array, the fewer stripes there are in a stripe set.  


Which keys must be pressed to access the PERC 2, 2/Si, 3/Si or 3/Di BIOS configuration utility?

   ALT A. 
 CRTL H. 
 CTRL A. **
 CRTL M. 

Question # 9 of 38

You have 153 minutes left (as of the time this page was requested from the server).

Mutliple choice:
How many channels are available for use on the PERC 2? 

   Six.  
 Two sets of four. 
 One. 
 Four. **


Question # 10 of 38

You have 151 minutes left (as of the time this page was requested from the server).

Multiple choice:
The PERC 2/Si RAID controller key is inserted into:

   PCI slot two. 
 The DRAC2 card. 
 The systemboard. ***
 The RAID controller card.  

Question # 11 of 38

You have 150 minutes left (as of the time this page was requested from the server).

True/False:
Initializing a drive from the PERC 2,2/Si, 3/Si, or 3/Di BIOS configuration utility deletes all data on the drive. 

   False. 
 True. **

Question # 12 of 38

You have 148 minutes left (as of the time this page was requested from the server).

Choose all that apply:
Do the following to activate the PERC 2/Si: 

   Remove the hard-disk drives.  
 Insert the RAID key into the system board. **
 Insert the RAID cache DIMM into the system board.  **
 Automaticlly activates upon installation. 

Question # 13 of 38

You have 147 minutes left (as of the time this page was requested from the server).

Multiple choice:
Which of the following describes the SCSI interface on the PERC 3/DCL, PERC 3/DC, and PERC 3/QC? 

   SCSI.  
 Ultra-3 SCSI.  **
 Ultra-2 SCSI (LVD).  
 SCSI-2.  

Question # 14 of 38

You have 146 minutes left (as of the time this page was requested from the server).

Choose all that apply:
The Perc 2/DC contains the following features: 

   Two channels. ***
 Four external SCSI connectors. 
 Two internal SCSI connectors. ***
 A cache battery. ***

Question # 15 of 38

You have 145 minutes left (as of the time this page was requested from the server).

True/False:
The PERC 2 contains four channels and six SCSI connectors. 

   False. 
 True. ***

Question # 16 of 38

You have 144 minutes left (as of the time this page was requested from the server).

True/False:
The PERC 2 RAID Controller BIOS configuration utility is entered by pressing Ctrl M. 

   False. ***
 True. 

Question # 17 of 38

You have 142 minutes left (as of the time this page was requested from the server).

Multiple choice:
The PERC 2/Si is an option in which Dell server(s)? 

   PE2400. ***
 PE6450. 
 PE4400. 
 PE2450. 

Question # 18 of 38

You have 138 minutes left (as of the time this page was requested from the server).

Choose all that apply:
Which of the following RAID controllers offer 128 MB of transportable battery-backed cache? 

   PERC 3/QC.  ***
 None of these selections.  
 PERC 3/DCL.  
 PERC 3/DC ***

Question # 19 of 38

You have 135 minutes left (as of the time this page was requested from the server).

True/False:
The PowerEdge 6450 supports embedded RAID. 

   False. ***
 True. 

Question # 20 of 38

You have 129 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What is the minimum service pack required to install Dell OpenManage Array Manager on a system running Microsoft Windows NT 4.0 Server Enterprise Edition?

   Service Pack 6a. 
 Service Pack 4.  
 Service Pack 3. ***
 Service pack 5. 

Question # 21 of 38

You have 129 minutes left (as of the time this page was requested from the server).

TRUE\FALSE:
With Dell OpenManage Array Manager's array policies can be edited from a remote station? 

   True **
 False 

Question # 22 of 38

You have 128 minutes left (as of the time this page was requested from the server).

Multiple Choice
What action must be taken to create a virtual disk from the menu tree in Array Manager?

   Double click a disk in the Disks folder. 
 Right click on a volume on the Volumes folder. 
 Right click on a disk in the Disks folder. 
 Right click on an Array group in the Array's folder. ***

Question # 23 of 38

You have 126 minutes left (as of the time this page was requested from the server).

Multiple Choice:
With Array Manager, the largest boot partition that can be configured is: 

   4096 MB.  ***
 9844 MB. 
 8644 MB. 
 1821 MB. 

Question # 24 of 38

You have 126 minutes left (as of the time this page was requested from the server).

Multiple Choice
When Array Manager is loaded on a system running Windows 2000 Server, what happens to the native disk management utility?

   The native uutilities functionality is combined with Array Manager. 
 The native utility operates in the backgroud. 
 Nothing, both can be used. 
 It is replaced by Array Manager. ***


Question # 25 of 38

You have 125 minutes left (as of the time this page was requested from the server).

TRUE\FALSE:
The more frequently the cache is flushed, the chances of data loss from a sudden loss of power is reduced. 

   True. ***
 False. 

Question # 26 of 38

You have 125 minutes left (as of the time this page was requested from the server).

Multiple chioce:
What is the purpose of expanding a virtual disk using Dell OpenManage Array Manager?

   To change disk type. 
 To decrease the size of an existing array. 
 To add a disk to an existing array. ***
 To recover from a failed drive. 

Question # 27 of 38

You have 124 minutes left (as of the time this page was requested from the server).

Choose all that apply:
What functions can be performed from the quick access menu in Dell OpenManage Array Manager? 

   Run Diagnostics. 
 Create a volume. **
 Set policies. 
 Remote Management.** 

Question # 28 of 38

You have 123 minutes left (as of the time this page was requested from the server).

Choose all that apply:
What must be specified when creating a virtual disk using Dell OpenManage Array Manager?

   Disk name. ***
 Set the permissions for the virtual disk to read only 
 The virtual disk size. 
 Format type. ***

Question # 29 of 38

You have 120 minutes left (as of the time this page was requested from the server).

TRUE\FALSE:
A designated hotspare configured when using an Adaptec PERC controller is individually assigned to each virtual disk.

   False. ***
 True. 

Question # 30 of 38

You have 117 minutes left (as of the time this page was requested from the server).

TRUE/FALSE
Array Manager supports AMI and Adaptec RAID controllers. 

   True. *** 
 False. 

Question # 31 of 38

You have 117 minutes left (as of the time this page was requested from the server).

Multiple Choice:
What is the purpose of converting from basic disk to dynamic disk?

   To create a software RAID volume. ***
 To remove any volumes on the basic disk. 
 To limit the number of volumes that can be created to four. 
 To provide access to data from Non-Microsoft operating systems. 

Question # 32 of 38

You have 116 minutes left (as of the time this page was requested from the server).

Multiple Choice:
The Array Manager Quick Acces menu can be used to view system configuration?

   False. 
 True. ***

Question # 33 of 38

You have 116 minutes left (as of the time this page was requested from the server).

TRUE\FALSE:
Dell OpenManage Array Manager manages storage resources on remote stations. 

   True. ***
 False. 

Question # 34 of 38

You have 116 minutes left (as of the time this page was requested from the server).

TRUE\FALSE:
Flushing the Cache on an AMI/LSI RAID controller means to take any information in the cache and write it to a hard disk. 

   False. 
 True. ***

Question # 35 of 38

You have 114 minutes left (as of the time this page was requested from the server).

TRUE\FALSE:
Adaptec and AMI/LSI RAID controllers offer the ability to designate a global Hot Spare that gets rebuilt if a drive fails. 

   False. 
 True. ***

Question # 36 of 38

You have 112 minutes left (as of the time this page was requested from the server).

Multiple Choice
What icon designates an unsigned disk in Dell OpenManage Array Manager?

   Yellow triangle with a black exclamation point. 
 White circle with a red X. 
 Red circle with a white bar. ***
 Green checkmark.  

Question # 37 of 38

You have 112 minutes left (as of the time this page was requested from the server).

Choose all that apply:
Which of the following can be selected when installing Management Station Applications? 

   Array Manager. 
 TCO Database Server. ***
 Remote Management. ***
 IT Assistant. 

Question # 38 of 38

You have 104 minutes left (as of the time this page was requested from the server).

Multiple Choice:
Which RAID levels can be changed with Dell OpenManage ArrayManger's online RAID level migration option when using an AMI/LSI PERC controller? 

   RAID 0 & 1 to RAID 5. 
 RAID 1 to RAID 5 & 0. 
 RAID 10 to RAID 5 & 0. 
 RAID 1 & 5 to RAID O. ***

The PERC 3/Si RAID controller key is located: 

   Above the PE4400 options bay. 
 On the PE2450 systemboard. ***
 On the PE4400 systemboard. 
 On the RAID controller card. 

Which of the following describes the PCI interface on the PERC 3/DCL, PERC 3/DC, and PERC 3/QC? 

   64-bit, 33 MHz.  
 64-bit, 66 MHz.  ***
 32-bit, 33 MHz.  
 Mini PCI.  

The PERC 2 RAID Controller contains six separate channels - four external and two internal. 

   True. 
 False. ***

When removing the PERC 2 RAID controller, the cache memory module must also be removed from the systemboard. 

   True. *
 False. 

What type of memory module is installed in the PERC 2/DC? 

   ECC SDRAM. ***
 EDO. 
 RIMM. 
 SIMM. 

In which Dell server(s) is the PERC 3/Di an option?

   PE1550. 
 PE2550. ***
 PE600SC. 
 PE4400. ***