DCSE Servers - PowerEdge 1655MC Product Certification (40 Questions)

True/False:
Each client workstation running the Remote Console Switch Software contains a local database that can be copied and loaded into other stations.
True.
False.

Multiple Choice:
What must be done to add a new server to an existing Remote Console Switch Software database?
Launch and complete the Update Wizard.
Nothing is required as it is automatically detected and added.
Launch and complete the Add New Server Wizard.
Launch and complete the Resync Wizard.

Choose All That Apply:
What steps must be performed to remove the hard-disk drives from the PowerEdge 1655MC?
Remove the server module.
Remove the midplane.
Open the server module.
Remove the memory.

Multiple Choice:
On the PowerEdge 1655, what must be removed before the power supplies can be removed from the chassis?
Server modules.
Hard-disk drives.
Switch modules.
Fans.

Multiple Choice:
On the PowerEdge 1655, what must be removed prior to removing the network switch modules?
The front bezel.
The hard-disk drives.
The rack rails.
Nothing.

True/False:
On the PowerEdge1655MC The AC power must be removed from the chassis before the microprocessor can be replaced in a server module.
False.
True.

Multiple Choice:
On the PowerEdge 1655MC, What must be done before the microprocessor can be removed from a server module?
Disconnect the AC power.
Remove the hard-disk drives.
Remove the server module.
Remove the memory.

Multiple Choice:
On the PowerEdge 1655MC, what must be removed before the systems management module can be removed?
Network switch modules.
Server module.
Fans.
Nothing.

True/False:
OSCAR must be used to upgrade an individual SIP's firmware.
True.
False.

Multiple Choice:
What should be done after a server module system board replacement to help avoid data loss on the PowerEdge 1655MC.
Reseat the hard-disk drive cables.
Nothing.
Boot to the PERC 4/IM mirror recovery diskette.
Install Windows 2000

True/False:
Managed nodes are the systems on a network that will be managed.
False.
True.

Choose all that apply:
What utilities are contained in the utility partition created using the Dell OpenManage Server Assistant CD?
Configuration Utility.
Server Diagnostics.
RAID Utility.
Server Administrator.

True/False:
The midplane on the PowerEdge 1655MC is hot swappable.
True.
False.

Choose all that apply:
On the PowerEdge 1655MC, what must be removed prior to removing the midplane?
System fans.
Server modules.
Power supplies.
system management and network switch modules.

True/False:
On the PowerEdge 1655MC server modules, the system setup can be accessed by pressing F12 during POST.
False.
True.

Multiple Choice:
The integrated PERC 4/IM in the PowerEdge 1655MC supports what Raid level.
RAID 3
RAID 1
RAID 50
RAID 0

Multiple Choice:
On the PowerEdge 1655MC, what keys must be pressed during post as the PERC 4/IM is recognized to enter the its configuration utility?
P + R.
Ctrl + M.
Alt+ X.
Esc + Alt.

True/False:
The integrated PERC 4/IM in the PowerEdge 1655MC supports Raid 50.
True.
False.

True/False:
System storage can be setup using the Dell OpenManage Array Manager Tool from the Dell OpenManage Server Assistant CD.
True.
False.

True/False:
On the PowerEdge 1655MC server modules, when booting to the PERC 4/IM recovery diskette using the USB floppy-disk drive the boot order must be manually changed in the system setup.
False.
True.

True/False:
On the PowerEdge 1655MC, when connected to the ERA/MC through HyperTerminal type connect switch-1 and press <Enter> to connect to switch module 1.
False.
True.

True/False:
On the PowerEdge 1655, A TFTP server is required to update the firmware on the ERA/MC.
True.
False.

Multiple Choice:
On the PowerEdge 1655MC, when connected to the ERA/MC through HyperTerminal what command is used to view the date and time on the ERA/MC.
racadm currenttime.
racadm gettime.
racadm getractime.
racadm time.

Multiple Choice:
On the PowerEdge 1655MC, when connected to the ERA/MC through HyperTerminal what command is used to set the date and time on the ERA/MC.
racadm setractime -d
racadm time
racadm getractime
racadm settime -d

Multiple Choice:
What service may need to be stopped in order for the TFTP server, used to upgrade the firmware on the PowerEdge 1655MC ERA/MC, to function?
Server service.
SNMP service.
OpForce service.
FTP service.

Multiple Choice:
On the PowerEdge 1655MC, when connected to the ERA/MC through HyperTerminal what command is used to get help on another ERA/MC command?
?.
help.
more.
info.

True/False:
Onboard NIC's can only be configured for DHCP during a Windows 2000 installation when using the Dell OpenManage Server Assistant CD.
False.
True.

True/False:
Onboard NIC's can only be configured for DHCP during a Windows 2000 installation when using the Dell OpenManage Server Assistant CD.
False.
True.

Multiple Choice:
What is the default password to login to IT Assistant with Read/Write rights?
Root.
Password.
Calvin.
A password does not exist by default.

True/False:
The Server Administrator application pull-down menu is only functional when two or more Dell OpenManage components are available on the managed system.
True.
False.

Choose all that apply:
What addressing specifications can be used to discover systems in IT Assistant?
IP address.
Netbui.
Host name.
IPX.

Choose All That Apply:
On the PowerEdge 1655MC, what interface options are available for management and configuration of the switch modules?
Server Administrator.
2161DS Remote Console Switch Software.
CLI.
OpenManage Switch Administrator.

Multiple Choice:
On the PowerEdge 1655MC, each switch module has how many external uplink Ethernet ports.
Four.
Two.
One.
Six.

True/False:
On the PowerEdge 1655MC, to connect to the switch modules at the ERA/MC prompt in the HyperTerminal window type, connect switch-1 or connect switch-2 and press the key.
True.
False.

Multiple Choice:
On the PowerEdge 1655MC, what command is used to copy the running configuration to the startup configuration on the network switch modules?
copy config startup-config.
move running-config startup-config.
copy running-config startup-config.
copy running-configuration startup-configuration.

Multiple Choice:
On the PowerEdge 1655MC switch module, what command is used to view the current IP address when using the CLI.
sh ip iaddress.
sh ip interface.
show ip info.
show ip interface.

True/False :
On the PowerEdge 1655MC, the switch modules support trunks participating in a VLAN.
False.
True.

True/False :
On the PowerEdge 1655MC, each switch module only supports one VLAN.
false.
True.

True/False:
On the PowerEdge 1655MC, the switch modules support dynamic as well as static trunks.
True.
False.

Multiple Choice:
On the PowerEdge 1655MC, what must be done prior to upgrading the firmware on the network switch modules?
Jumper JP6 will need to be moved form Pins 1 and 2 to pins 2 and 3
The ERA/MC will need to be removed from the chassis..
All Ethernet cables will need to be disconnected.
Nothing.

True/False:
The PowerEdge 1655MC supports having a PowerVault 210/211S connected directly to the chassis.
True.
False.

Choose all that apply:
What ports are used by the PowerEdge 2161DS and the Dell Remote Console Switch Software?
8192.
21.
2068.
3211.

True/False:
The PowerEdge 2161DS must have an IP address assigned to it prior to installing the Remote Console Switch Software.
False.
True.

Choose All That Apply:
What steps must be performed to remove the hard-disk drives from the PowerEdge 1655MC?
Remove the server module.
Remove the midplane.
Open the server module.
Remove the memory.

Multiple Choice:
On the PowerEdge 1655, what must be removed before the power supplies can be removed from the chassis?
Hard-disk drives.
Fans.
Server modules.
Switch modules.

Multiple Choice:
On the PowerEdge 1655, what must be removed prior to removing the network switch modules?
The rack rails.
The front bezel.
The hard-disk drives.
Nothing.

Multiple Choice:
On the PowerEdge 1655MC, What must be done before the microprocessor can be removed from a server module?
Remove the memory.
Remove the hard-disk drives.
Disconnect the AC power.
Remove the server module.

Multiple Choice:
On the PowerEdge 1655MC, what must be removed before the systems management module can be removed?
Nothing.
Fans.
Server module.
Network switch modules.

True/False:
OSCAR must be used to upgrade an individual SIP's firmware.
False.
True.

Multiple Choice:
What should be done after a server module system board replacement to help avoid data loss on the PowerEdge 1655MC.
Reseat the hard-disk drive cables.
Nothing.
Boot to the PERC 4/IM mirror recovery diskette.
Install Windows 2000

Choose all that apply:
What CD-ROMs comprise the Dell OpenManage Installation program?
Connection Agent.
Systems Management.
Documentation.
Server Assistant.

Choose all that apply:
What utilities are contained in the utility partition created using the Dell OpenManage Server Assistant CD?
Server Administrator.
RAID Utility.
Server Diagnostics.
Configuration Utility.

True/False:
The midplane on the PowerEdge 1655MC is hot swappable.
False.
True.

True/False:
On the PowerEdge 1655MC server modules, the system setup can be accessed by pressing F12 during POST.
False.
True.

Multiple Choice:
The integrated PERC 4/IM in the PowerEdge 1655MC supports what Raid level.
RAID 0
RAID 3
RAID 50
RAID 1

True/False:
The integrated PERC 4/IM in the PowerEdge 1655MC supports mirroring.
True.
False.

True/False:
Windows 2000 Service Pack 3 is contained on the Dell OpenManage Server Assistant CD ver. 7.2.3.
True.
False.

Multiple Choice:
On the PowerEdge 1655MC, when connected to the ERA/MC through HyperTerminal what command is used to set the date and time on the ERA/MC.
racadm time
racadm getractime
racadm setractime -d
racadm settime -d

True/False:
On the PowerEdge 1655MC server modules, when booting to the PERC 4/IM recovery diskette using the USB floppy-disk drive the boot order must be manually changed in the system setup.
True.
False.

True/False:
On the PowerEdge 1655MC, A null modem cable is used to create the connection between the ERA/MC and the client system for configuration.
True.
False.

Multiple Choice:
What service may need to be stopped in order for the TFTP server, used to upgrade the firmware on the PowerEdge 1655MC ERA/MC, to function?
OpForce service.
SNMP service.
Server service.
FTP service.

True/False:
On the PowerEdge 1655, A TFTP server is required to update the firmware on the ERA/MC.
True.
False.

Multiple Choice:
On the PowerEdge 1655MC, when connected to the ERA/MC through HyperTerminal what command is used to get help on another ERA/MC command?
more.
?.
info.
help.

Multiple Choice:
On the PowerEdge 1655MC, when connected to the ERA/MC through HyperTerminal what command is used to view the date and time on the ERA/MC.
racadm getractime.
racadm gettime.
racadm time.
racadm currenttime.

True/False:
On the PowerEdge 1655MC, when connected to the ERA/MC through HyperTerminal type connect switch-1 and press <Enter> to connect to switch module 1.
False.
True.

True/False:
The SNMP community name cannot be specified during a Windows 2000 installation when using the Dell OpenManage Server Assistant CD.
True.
False.

True/False:
Server Administrator can be accessed both locally and remotely.
True.
False.

Multiple Choice:
What is a image server?
The PowerEdge 1655MC Blades.
Any Dell PowerEdge Server running Red Hat Linux 7.3.
Any desktop system running Windows 2000.
Any Dell PowerEdge Server running Windows 2000.

Multiple Choice:
What is a target system?
Any desktop system running Windows 2000.
The PowerEdge 1655MC Blades.
Any Dell PowerEdge Server running Windows 2000.
Any Dell PowerEdge Server running Red Hat Linux 7.3.

Multiple Choice:
On the PowerEdge 1655MC, each switch module has how many Ethernet ports connected internally to the midplane.
Eleven.
Ten.
Twelve.
Six.

Multiple Choice:
On the PowerEdge 1655, what is the maximum speed supported by the ports on the netweok switch modules?
1000 Mbps.
16 Mbps.
100 Mbps.
10 Mbps.

Choose All That Apply:
On the PowerEdge 1655MC, what interface options are available for management and configuration of the switch modules?
2161DS Remote Console Switch Software.
Server Administrator.
CLI.
OpenManage Switch Administrator.

True/False:
On the PowerEdge 1655MC, the default login for the switch modules is admin.
False.
True.

Multiple Choice:
On the PowerEdge 1655MC switch module, what command is used to view the current IP address when using the CLI.
show ip interface.
sh ip iaddress.
show ip info.
sh ip interface.

Multiple Choice:
On the PowerEdge 1655MC, what command is used to copy the running configuration to the startup configuration on the network switch modules?
move running-config startup-config.
copy config startup-config.
copy running-config startup-config.
copy running-configuration startup-configuration.

True/False :
On the PowerEdge 1655MC, the switch modules support trunks participating in a VLAN.
False.
True.

On the PowerEdge 1655MC, each switch module only supports one VLAN.
True.
false.

True/False:
On the PowerEdge 1655MC, the switch modules support dynamic as well as static trunks.
True.
False.

Multiple Choice:
On the PowerEdge 1655MC, what must be done prior to upgrading the firmware on the network switch modules?
All Ethernet cables will need to be disconnected.
Jumper JP6 will need to be moved form Pins 1 and 2 to pins 2 and 3
The ERA/MC will need to be removed from the chassis..
Nothing.

True/False:
The PowerEdge 1655MC supports having a PowerVault 210/211S connected directly to the chassis.
True.
False.