What is the proper procedure to follow if the customer has a PowerVault 530F in their SAN?

   Do not perform any upgrade procedures. Use standard escalation procedures. *
 Upgrade all components in the SAN other than the PowerVault 530F. 
 Insert the PowerVault 530F Upgrade disk into the PowerVault 530F. Click Appliance Upgrade. When prompted, reboot the appliance. 
 Insert the PowerVault 530F Upgrade disk into the PowerVault 530F and reboot the SAN appliance. 

How do you determine the version of StorageC that is installed?

   The version is listed in the service name. 
 The version is returned by the storagec info command line. This needs to be run from the c:\program files\openmanage\storage consolidation path. 
 The version can not be determined. 
 The version is returned by the storagec -version command line. This needs to be run from the c:\program files\openmanage\storage consolidation path. *

Question # 17 of 19

You have 69 minutes left (as of the time this page was requested from the server).

What is the proper procedure to follow if you are replacing a RAID controller in a PowerVault 660F and the firmware revision on the replacement controller is different than the working controller?

   Determine what firmware revision the surviving RAID controller is and flash the replacement controller to match. *
 Upgrade and replace as appropriate. 
 Do not replace the RAID controller. Call technical support. 
 Downgrade and replace as appropriate. 

Question # 16 of 19

You have 69 minutes left (as of the time this page was requested from the server).

What services must be stopped before upgrading the Qlogic Configuration Utility?

   Only the Win32SL needs to be stopped. 
 No services need to be stopped. 
 Before installing Qlconfig the QLConfig NT Agent service and the Win32SL service must be stopped. *
 Only the QLCOnfig NT Agent service needs to be stopped. 
 Flag for review


Question # 15 of 19

You have 70 minutes left (as of the time this page was requested from the server).

Multiple Choice:
Which of the following best describes the function of Dell OpenManage Data Managed Node (Data Agent)?

   Provides data path failover for a server connected to a Dell PowerVault 65xF disk enclosure in a redundant configuration. 
 Establishes and manages data paths between servers and devices in the Fibre Channel SAN. 
 Serves as an SNMP proxy to help allow a server to configure and manage a Dell PowerVault 65xF disk enclosure. *
 Provides a GUI management interface that is used to configure and manage a Dell PowerVault 65xF disk enclosure. 

 Question # 14 of 19

You have 70 minutes left (as of the time this page was requested from the server).

Multiple Choice:
Which of the following best describes the function of the QLogic Fibre Channel Configuration Utility (QLconfig)?

   Provides data path failover for a server connected to a Dell PowerVault 65xF disk enclosure in a redundant configuration.  
 Serves as an SNMP proxy to help allow a server to configure and manage a Dell PowerVault 65xF disk enclosure. 
 Establishes and manages data paths between servers and devices in the Fibre Channel SAN. *
 Allows the OS to use and control the QLogic Fibre Channel HBA.  

Question # 13 of 19

You have 71 minutes left (as of the time this page was requested from the server).

Multiple Choice:
Which of the following best describes the function of Dell OpenManage Storage Consolidation (Storage C)?

   Protects data by providing LUN masking for Microsoft Windows NT 4.0 and Microsoft Windows 2000 operating systems. *
 Serves as an SNMP proxy to help allow a server to configure and manage a Dell PowerVault 65xF disk enclosure. 
 Establishes and manages data paths between servers and devices in the Fibre Channel SAN. 
 Provides a GUI management interface that is used to configure and manage a Dell PowerVault 65xF disk enclosure. 

Which of the following best describes the function of Dell OpenManage Application Transparent Failover (ATF)?

   Establishes and manages data paths between servers and devices in the Fibre Channel SAN. 
 Provides a GUI management interface that is used to configure and manage a Dell PowerVault 65xF disk enclosure. 
 Protects data by providing LUN masking for Microsoft Windows NT and Microsoft Windows 2000 operating systems. 
 Provides data path failover for a server connected to a Dell PowerVault 65xF disk enclosure in a redundant configuration.  *

Question # 11 of 19

You have 71 minutes left (as of the time this page was requested from the server).

After flashing the RAID controllers Array manager reports that the enclosure did not respond to the reboot command. What is the most likely cause?

   This indicates that disks 0 through 3 have gone offline. Click , perform a re-scan, and issue another reboot command. 
 This is normal. The proper procedure is to power cycle the enclosure. *
 The flash has failed. Reflash the enclosure. 
 This indicates a timeout condition. Click <Cancel>, perform a refresh and issue another reboot command. 


 
  Flag for review 


Question # 10 of 19

You have 73 minutes left (as of the time this page was requested from the server).

After flashing the RAID controllers and rebooting the enclosure, the enclosure never completes POST. What is the most likely cause?

   The firmware flash to one of the RAID controllers has probably failed and now the two RAID controllers are at different firmware revisions. This will prevent the enclosure from completing POST. 
 This indicates a power supply failure. 
 A firmware incompatibility exists between the RAID controllers and the LS Modules. The LS Modules should always be flashed prior to flashing the RAID controllers. *
 One of the RAID controllers has failed to power up. This is also known as a “partner failed condition”. 


 
  Flag for review 
What is the difference between part number 1G987 and part number 8K166?

   Part number 1G987 is a PowerVault 660F RAID controller that ships with 7.51 firmware. 
Part number 8K166 is a PowerVault 660F RAID controller that ships with 7.70 firmware. 
 There is no difference. 
 Part number 1G987 is a PowerVault 660F RAID controller that ships with 7.70 firmware. *
Part number 8K166 is a PowerVault 660F RAID controller that ships with 7.51 firmware. 
 1G987 is a PowerVault 660F RAID controller that ships without a firmware flash diskette. 
8K166 is a PowerVault 660F RAID controller that ships with a firmware flash diskette. 


 
  Flag for review 

Question # 8 of 19

You have 73 minutes left (as of the time this page was requested from the server).

On the PowerVault 660F, how does the World Wide Name propagation differ between the 7.51 RAID controller firmware and the 7.70 RAID controller firmware?

   In the 7.51 firmware the WWN propagates from the secondary controller to the primary controller. In the 7.70 firmware the WWN propagates from the backplane to both controllers. 
 The WWN propogates the same way in both firmware versions. *
 In the 7.51 firmware the WWN propagates from the primary controller to the secondary controller. In the 7.70 firmware the WWN propagates from the backplane to both controllers. 
 In the 7.70 firmware the WWN propagates from the primary controller to the secondary controller. In the 7.51 firmware the WWN propagates from the backplane to both controllers. 


 
  Flag for review 
Which of the following is the most likely cause for not being able to see the graphical screens in the Dell Switch Manager?

   Dell Switch Manager has not been installed. 
 The FC-AL address for the switch has been set incorrectly. 
 The system being used to access the switch does not have the Sun JavaSoft Java 1.2.2 browser plug-in installed. *
 The system accessing the switch is not a member of any Zone on the switch. 

Which of the following is the most likely to cause a DEFAULT STORAGE GROUP to appear in the Storage C Administrator?

   Dell OpenManage Storage Consolidation has not been installed on one or more servers in the SAN. 
 All of the servers and storage devices in the SAN are configured with factory defaults. 
 No servers have been configured as the MASTER from Storage C Administrator. 
 Data paths have not been configured between some of the servers and storage devices. *

Which of the following best describes the function of QLDirect?

   Provides a GUI management interface that is used to configure and manage a Dell PowerVault 660F disk enclosure. 
 Provides data path failover for a server connected to a Dell PowerVault 660F storage system in a redundant configuration. *
 Allows the OS to use and control the QLogic Fibre Channel HBA. 
 Establishes and manages data paths between servers and devices in the Fibre Channel SAN. 

 Which of the following is used to configure virtual disks and perform management operations on the Dell PowerVault 660F?

   Dell OpenManage Data Managed Node. 
 Dell OpenManage Data Management Station. 
 Dell OpenManage Array Manager version 2.7.1 or later. *
 Dell OpenManage Storage Consolidation. 

Multiple Choice:
Which of these should be configured prior to installing Dell OpenManage Storage Consolidation (Storage C)?
I. - Common Domain Membership.
II. - TCP/IP name resolution (hosts file or DNS).

   Both I and II. *
 II only. 
 I only. 
 Neither I nor II. 

What is the installation procedure for the Dell Switch Manager?

   There is no installation procedure. The Dell Switch Manager is a feature of the switch firmware (Fabric OS). *
 The Dell Switch Manager is installed as a component of Dell OpenManage Data Management Station. 
 The Dell Switch Manager is installed as a component of the QLogic Fibre Channel Configuration Utility. 
 Select Dell Switch Manager from the main menu on the SAN 3.0 Fibre Channel Update CD. 

 Which of the following is an end point in the simplified Fibre Channel data flow model?

   Fibre Channel switch. 
 Physical Media or Cabling. 
 A LUN on a Dell PowerVault DPE. *
 The QLogic HBA(s) in a server. 

84%
 



