Which CLI command will display the list of aliases and zones on a PowerVault 51/56F?

   ShowAli.  
 ShowAlias.  
 AliShow.  *
 MapAli. 

What tool could you use to verify fibre channel communication? 

   Array Manager. 
 QLCONFIG.  *
 Array Manager Service Manager.  
 PowerVault Administrator. *

In a World Wide Name, what do the 4th and 5th bytes with a value of 60:16 denote? 

   Dell PowerVault 5xF Fibre Channel Switch.  
 Dell PowerVault 65xF Fibre Channel DPE.  *
 Dell PowerVault 35F Fibre Channel Bridge.  
 Dell PowerVault 660F Storage System.  
 
You have 57 minutes left (as of the time this page was requested from the server).

True/False:
A PowerVault 136T must be connected to a SAN using a PowerVault 35F.

   False. *
 True. 

A special tape library module must be installed for a PowerVault 136T to be controlled by Veritas Backup Exec 8.x.

   True. *
 False. 

Veritas Backup Exec 8.5 can use its own drivers to perform backups. 

   True. 
 False. *

When can 'Cable Analysis' be tested on a Broadcom NIC using the BASCS utility?

   When connected to a gigabit switch.  *
 Cable Analysis cannot be tested. 
 When connected to a 100 Mbps switch.  
 When connected to an autosensing 10/100 switch.  

Broadcom adapters support Adapter Fault Tolerance (AFT), Adapter Load Balancing (ALB), and Virtual LANs (VLANs). 

   True. *
 False. 

Which is a Hot Plug PCI type? 

   Hot Upgrade. *
 Hot Replacement. *
 Hot Transfer. 
 Hot Addition. *

On a PowerEdge 6400, a hot swappable PCI card may be safely removed from the PCI slot only when the green LED is lit.

   False. *
 True. 

Adapter Load Balancing (ALB) provides what other function? 

   FEC (Fast Ethernet Channel) Access. 
 AFT (Adapter Fault Tolerance). *
 VLAN (Virtual LAN). 
 NIC (Network Interface Coordination). 

What is the name of the software used to configure adapter teaming for Intel NICs?

   Intel Adapter software. 
 None adapter teaming is done through the adapters BIOS. 
 Intel Adapter Configurator.  
 Intel PROSet. *

What is a TAM? 

   Total Accountability Manager. 
 Technical Accuracy Manager.  
 Technical Account Manager.  *
 Troubleshooting Account Manager.  

You have come across an accurate and reliable non-Dell diagnostic tool. It is permissable to use this tool while performing onsite troubleshooting at a customer's site.

   False. *
 True. 

What tasks can be performed using the Dell Library & Tape Tools utility? 

   Test a device.  *
 Perform a system backup.  
 Schedule a backup.  
 Upgrade firmware.  *

What is the icon color of a supported device in the Dell Library & Tape Tools utility?

   Green. 
 Blue. *
 All devices are the same color, supported or not. 
 Red. 

In Array Manager, a logical drive is defined as: 

   An abstract entity made up of disks and/or disk segments.  
 A disk that adheres to the partition oriented scheme of Windows NT, 9x and MS-DOS.  
 A disk controlled by a RAID controller.  
 A simple volume that resides on an extended partition of a basic disk.  *

What is the maximum number of Virtual Disks a PERC3/QC controller will support? 

   8 
 40. *
 24. 
 18. 

Which of the following can be used to try and repair a corrupted Windows 2000 Server OS installation?

   Express Installation with the DSA.  
 Emergency Repair Process  *
 Safe Mode.  *
 Recovery Console. *

The Recovery Console can be installed as a boot option. 

   False. 
 True. *

You can keep a log of results when performing Dell Diagnostics. 

   False. 
 True. *

What are the test modes for the ELITE diagnostics? 

   Fullscan mode.  *
 Standard mode.  
 Normal mode.  *
 Fast mode.  

How many troubleshooting steps were discussed in class? 

   Five. *
 Six. 
 Four. 
 Three. 

When you have finished a troubleshooting call, what must be done before you can leave the site?

   Contact the EEC for authorization to leave. 
 Make copies of the event log(s). 
 Show the customer the problem has been resolved. *
 Call technical support to close the call. *

88% Good luck!!



 










