Storage - PowerVault 110T SDLT 220 and SDLT 320 Product Certification

There are 7 questions, you have 28 minutes.

Multiple Choice
The native backup storage capacity of the PV110T SDLT320 is:
110MB.
160MB.
320KB.
320MB.

True/False:
A low voltage differential terminator should be used to terminate the SCSI chain on the back of the PV110T SDLT/SDLT320.
True.
False.

True/False:
A low voltage differential terminator should be used to terminate the SCSI chain on the back of the PV110T SDLT/SDLT320.
True.
False.

Multiple choice:
When installing a PV110T SDLT220 or SDLT320, a ball-point pen is used to:
Set the date and time.
Label the tape.
Set the SCSI ID.
Write down the service tag number.

Multiple choice
When setting up the PV110T SDLT tape drive, set the SCSI ID to any of the following numbers:
3.
9.
16.
7.

True/false
Veritas Backup Exec version 8.6 is supported on the PV110T SDLT 320 tape drive.
False.
True.

Multiple choice
What tool is used to remove the tape drive leader pin from the cartridge buckle in the PV110T SDLT tape drive?
Needle-nose pliers.
Tweezers.
#1 Phillips-head screw driver.
Magnetic screw-driver.