Storage – PowerVault 120T DLT1 Autoloader Certification

There are 15 questions, you have 60 minutes.

Multiple choice:
The PowerVault 120T DLT1 Autoloader writes and reads DLT tapes with a maximum density of:
40 GB.
70 GB.
80 MB.
80 GB.

True/False:
The PowerVault 120T DLT1 Autoloader is configured as a table top or a rack mount unit.
False.
True.

Multiple choice:
The PowerVault 120T DLT1 Autoloader can read tapes that were written by the:
PV130T.
DLT7000.
PV110.
DLT4000.

Multiple choice:
The PowerVault 120T DLT1 Autoloader is attached to a controller using the following technology:
HVD SCSI.
LVD SCSI.
IDE.
SCSI Ultra Narrow.

True/False:
The PowerVault 120T DLT1 Autoloader whole unit is a field replaceable unit (FRU).
True.
False.

Choose all that apply:
The PowerVault 120T DLT1 Autoloader attaches to the following SCSI controller:
Adaptec 7860.
AHA-39160.
Adaptec 7933.
Adaptec AIC 7899.

Choose all that apply:
The PowerVault 120T DLT1 Autoloader contains the following SCSI devices:
The SCSI controller.
The DLT tape drive.
The SCSI backplane.
The robotics.

Choose all that apply:
On the PowerVault 120T DLT1 Autoloader, use the following tools to remove a stuck tape in an emergency situation:
Flat-blade screwdriver.
#1 Phillips screw driver.
3/8 inch nut driver.
9-Volt battery.

Choose all that apply:
Before checking for connectivity with the server on a new PowerVault 120T DLT1 Autoloader, do the following:
Attach the PowerVault 120T DLT1 Autoloader to the server.
Check the SCSI IDs with the SCSI utilities on the server.
Attach the SCSI cable to the Adaptec 7933 controller.
Run the device self-test.

Multiple choice:
The second rack-mount PowerVault 120T DLT1 Autoloader unit is secured to the first unit with:
A locking bar.
Three phillips-head screws.
The rack mounting rail slide.
One screw.

Choose all that apply:
Before installing the PowerVault 120T DLT1 Autoloader, perform the following steps first:
Verify that the customer has the correct power outlets.
Remove the packing material inside the PowerVault 120T DLT Autoloadeer.
Install a DLT tape.
Attach the SCSI terminator.

Multiple choice:
If the PowerVault 120T DLT1 Autoloader is the last device on a SCSI bus, a terminator with the following label must be attached to the empty 68-pin slot on the rear of the system:
LVD Terminator.
HVD Terminator.
IDE Terminator.
HPPCI Terminator.

True/False:
You must wait for LdR REAdY to be displayed on the front LCD panel before installing DLT tapes in the PowerVault 120T DLT1 Autoloader.
False.
True.

Multiple choice:
When replacing a PowerVault 120T DLT1 Autoloader, the service tag plate is transferred to the new unit and secured with:
Two rivets.
Super glue.
A pressure sensitive label.
Two Phillips-head screws.

Multiple choice:
On the PowerVault 120T DLT1 Autoloader, Data cartridges for slots six and seven are loaded from slots:
One and two.
Three and four.
Four and Five.
Six and seven.