Array Manager supports AMI and Adaptec RAID controllers. 

   False. 
 True.  *

What icon designates an unsigned disk in Dell OpenManage Array Manager?

   White circle with a red X. 
 Green checkmark.  
 Yellow triangle with a black exclamation point. 
 Red circle with a white bar. *

What functions can be performed from the quick access menu in Dell OpenManage Array Manager? 

   Set policies. 
 Create a volume. *
 Run Diagnostics. 
 Remote Management. *

Which RAID levels can be changed with Dell OpenManage ArrayManger's online RAID level migration option when using an AMI/LSI PERC controller? 

   RAID 1 & 5 to RAID O. *
 RAID 1 to RAID 5 & 0. 
 RAID 10 to RAID 5 & 0. 
 RAID 0 & 1 to RAID 5. 

Flushing the Cache on an AMI/LSI RAID controller means to take any information in the cache and write it to a hard disk. 

   True. *
 False. 

The rebuild rate option determines the percentage of the systemboard processor's capacity to be rebuild a virtual disk.

   False. *
 True. 

What must be specified when creating a virtual disk using Dell OpenManage Array Manager?

   The virtual disk size. *
 Format type. ???
 Set the permissions for the virtual disk to read only 
 Disk name. *

Dell OpenManage Array Manager manages storage resources on remote stations with the following operating system: 

   Windows 98. 
 Windows 2000 Advanced Server. *
 Netware 5.0. 
 NT 4.0 Server. *

Which of the following components can be selected during installation of the Dell Open Manage Array Manager's, Managed Node services? 

   Version Management. *
 TCO Management. 
 Server Diagnostics.* 
 RAID Management. *

The Array Manager Quick Acces menu can be used to view system configuration?

   False. 
 True. *

Which of the following can be selected when installing Management Station Applications? 

   IT Assistant. *
 TCO Database Server. 
 Remote Management. 
 Array Manager. *

What action must be taken to create a virtual disk from the menu tree in Array Manager?

   Double click a disk in the Disks folder. 
 Right click on a volume on the Volumes folder. 
 Right click on a disk in the Disks folder. 
 Right click on an Array group in the Array's folder. *

When Array Manager is loaded on a system running Windows 2000 Server, what happens to the native disk management utility?

   The native uutilities functionality is combined with Array Manager. 
 The native utility operates in the backgroud. 
 Nothing, both can be used. 
 It is replaced by Array Manager. *

TRUE\FALSE:
With Dell OpenManage Array Manager's array policies can be edited from a remote station? 

   True 
 False *

Array Manager manages arrays on all Dell products.

   True *
 False 

Dell OpenManage Array Manager manages storage resources on remote stations. 

   False. *
 True. 

With Array Manager, the largest boot partition that can be configured is: 

   1821 MB. 
 8644 MB. (should be this)
 4096 MB.  *???
 9844 MB. 


The more frequently the cache is flushed, the chances of data loss from a sudden loss of power is reduced. 

   False. 
 True. *

What is the purpose of expanding a virtual disk using Dell OpenManage Array Manager?

   To decrease the size of an existing array. 
 To change disk type. 
 To recover from a failed drive. 
 To add a disk to an existing array. *

The PERC 3/Si cache memory is inserted into: 

   The RAID controller card. 
 The systemboard. *
 PCI slot three. 
 Server system memory slot four. 

The PERC 3/Di BIOS configuration utility is entered by pressing: 

   Ctrl Z.  
 Ctrl M. 
 Alt A. 
 Ctrl A. *

Do the following to activate the PERC 2/Si: 

   Insert the RAID key into the system board. *
 Remove the hard-disk drives.  
 Automaticlly activates upon installation. 
 Insert the RAID cache DIMM into the system board.  *

Which of the following describes the SCSI interface on the PERC 3/DCL, PERC 3/DC, and PERC 3/QC? 

   SCSI-2.  
 Ultra-2 SCSI (LVD).  
 SCSI.  
 Ultra-3 SCSI.  *

The PERC 2 RAID Controller BIOS configuration utility is entered by pressing Ctrl M. 

   False. 
 True. *

The PERC 2/Si is an option in which Dell server(s)? 

   PE2450. 
 PE6450. 
 PE2400. *
 PE4400. 

The PERC 2 contains four channels and six SCSI connectors. 

   False. 
 True. *

The PERC 3/DC and PERC 3/QC can retain cache data for up to 72 hours. 

   True. *
 False. 

In which Dell server(s) is the PERC 3/Di an option?

   PE2550. *
 PE1550. 
 PE600SC. 
 PE4400. *

Which keys must be pressed to access the PERC 2, 2/Si, 3/Si or 3/Di BIOS configuration utility?

   CTRL A. *
 CRTL H. 
 ALT A. 
 CRTL M. 
 
Which of the following describes the PCI interface on the PERC 3/DCL, PERC 3/DC, and PERC 3/QC? 

   64-bit, 33 MHz.  
 32-bit, 33 MHz.  
 64-bit, 66 MHz.  *
 Mini PCI.  

The PERC 3/Di cache memory DIMM is located: 

   In the PE4400 system memory slot four. 
 On the RAID controller card. 
 On the PE4400 systemboard. *
 On the PE2450 systemboard. 
 
You should choose a RAID 10 configuration to combine the: 

   Fault tolerance of RAID 1 with the performance of RAID 0.  *
 Fault tolerance of RAID 5 with the performance of RAID 0.  
 Storage efficiency of RAID 1 with the fault tolerance of RAID 0.  
 Performance of RAID 5 with the fault tolerance of RAID 0. 

When should a RAID 1 configuration be used?

   There is a large budget and the need to process large digital video files at high speeds.  
 There is a limited budget and the ability to recover all critical information from tape backups.  
 When there is a large budget and requirement to accept multiple simultaneous requests for access. 
 For small databases or any other environment that requires fault tolerance but small capacity.  *

The acronym 'RAID' stands for:

   Reliable Array of Inexpensive Drives. 
 Reliable Array of Inexpensive Disks. 
 Redundant Array of Interconnected Disks. 
 Redundant Array of Independent Disks. *
 
Which of the following statements describes a stripe set? 

   A stripe set stores a different file in each stripe. 
 The sizes of stripes in a stripe set are the same.  *
 The more disks there are in an array, the fewer stripes there are in a stripe set.  
 A disk is reserved for all the stripes in a stripe set. 

Which of the following statements describe RAID 5?

   Data stripes are interleaved with parity stripes over disks.  *
 Data stripes are interleaved while parity stripes are placed on a specified disk.  
 Data stripes are interleaved over one half of the drive array while parity stripes are placed on the other half. 
 Data stripes and parity stripes alternate within a stripe set over disks that are synchronized. 

What RAID level does NOT provide fault tolerance?

   RAID 3. 
 RAID 0. *
 RAID 1. 
 RAID 5. 

Dell OpenManage Array Manager 3.1.2 must be installed prior to installing Dell OpenManage Hard Drive Diagnostics to detect and test devices attached to a RAID controller. 

   True. *
 False. 


87%


 







