To change the IP address on the PV128T LTO Library, the global service password must be entered first via the operator panel.

   True. ***
 False. 

The PV128T LTO Tape Library can store up to ________ LTO tape cartridges.

   19. 
 20. ***
 10. 
 72. 

Attaching the PV128T LTO Tape Library to a SAN is accomplished through the:

   RMC. 
 SCSI host adapter. 
 Fibre Channel Card. ***
 Library controller card. 

LTO tape cartridges are loaded into the tape drive modules in the PV128T LTO Tape Library through the:

   Power supply. 
 Magazines. 
 Library controller card. 
 Transport assembly ***

The PV128T LTO Tape Library must be attached to an external PowerVault 35F to attach the library to a SAN.

   True. 
 False. ***

The library and tape tools program can be used to upgrade firmware on the PV128T LTO Tape Library.

   False.  
 True. ***

The SCSI connector assembly is secured to the tape drive modules on the 128T LTO tape Library with:

   A SCSI connector. 
 Two thumbscrews. ***
 The SCSI cable. 
 A flat-blade screwdriver. 

The system board on the PV128T LTO Tape Library can be removed while the library is installed in a rack.

   False. 
 True. ***

Choose all that apply
Perform the following before removing the transport assembly from the PV128T LTO Tape Library:

   Remove the standalone cover. ***
 Use the back handle to push it to the maintenance position in a rack. ***
 Disconnect the AC power cable. ***
 Remove it from the rack and place on a flat surface. 

The magazine slide tray on the PV128T LTO Tape Library is secured with:

   Four T8 torx screws.  
 Six T15 torx screws. ***
 The magazine lock assembly. 
 The mailslot solenoid assembly. 

To remove the library controller card on the PV128T LTO Tape Library, use the following:

   A T10 torx driver. 
 A Phillips-head screwdriver. ***
 A 1/4 inch nut driver. 
 Your fingers. ***

Before removing the display panel assembly on the PV128T LTO Tape Library, remove the:

   Tape drive modules.  
 Magazines. ***
 Display window frame.*** 
 Bezel chin. ***

The PV128T LTO Tape Library fibre channel card contains:

   A copper fibre channel connector. 
 An optical fibre channel connector. ***
 Two GBICs. 
 One GBIC. 


100%




