Servers - PowerEdge 2650 Product Certification (36 Questions)

Multiple Choice:
What must be removed prior to removing the hard-disk drives from the PowerEdge 2650?
The system cover.
The CD-ROM.
The backplane.
The front bezel.

Multiple Choice:
On the PowerEdge 2650, where are the three thumbscrews located that secure the system cover to the chassis?
On the back of the system.
On the front of the system.
On the left side of the system.
On the right side of the system.

Multiple Choice:
On the PowerEdge 2650, what must be removed prior to removing the floppy-diskette/CD-ROM/DVD-ROM drive assembly?
System cover.
Front bezel.
Hard-disk drives.
Rack rails.

Multiple Choice:
On the PowerEdge 2650, how many cables must be disconnected from the back of the CD-ROM/DVD-ROM drive?
One.
Four.
Two.
Three.

Choose all that apply:
What must be removed prior to removing the control panel from the PowerEdge 2650?
All hard-disk drives.
The system cover.
The CD-ROM.
The front bezel.

Multiple Choice:
On the PowerEdge 2650, how many cables must be disconnected from the control panel prior to removing the control panel?
Four.
One.
Two.
Three.

Multiple Choice:
On the PowerEdge 2650, how many cables must be disconnected from the back of the floppy-diskette drive?
Three.
Four.
Two.
One.

Multiple Choice:
On the PowerEdge 2650, the power supply must be removed from _______ of the system.
Right side.
Left side.
Back.
Front.

Multiple Choice:
On the PowerEdge 2650, where is the control-panel cable cover release tab located?
Next to the chassis wall.
Next to the control panel.
Next to the expansion card cage.
Next to the split backplane card.

Multiple Choice:
On the PowerEdge 2650, what FRU must the front panel I/O board be disconnected from?
Split backplane card.
Backplane.
Control panel board.
Power distribution board.

Multiple Choice:
Where is the split backplane card located on the PowerEdge 2650?
Next to the expansion card cage.
Below the hard-disk drives.
Above the middle hard-disk drive bay.
On the system board.

True/False:
On the PowerEdge 2650, to release the system board tray from the chassis, you must rotate the system board tray levers up simultaneously.
True.
False.

Multiple Choice:
On the PowerEdge 2650, where are the system board tray levers located?
Under the system board.
Behind the system fan bracket.
On the front of the system chassis.
Behind the backplane.

True/False:
On the PowerEdge 2650, you must loosen a single thumbscrew to remove the backplane from the system chassis?
True.
False.

Multiple Choice:
On the PowerEdge 2650, how many fans are installed if the system is configured with a single processor?
Four.
Three.
Six.
Five.

Choose all that apply:
On the PowerEdge 2650, what must be removed prior to removing the system fan bracket?
Front bezel.
System board tray.
System cover.
The two fans at the back of the system.

True/False:
On the PowerEdge 2650, you must loosen the two thumbscrews that secure the expansion-card cage to the chassis in order to remove the expansion card cage?
True.
False.

True/False:
On the PowerEdge 2650, a metal filler bracket must be installed over any empty expansion slot opening to maintain proper cooling and airflow.
True.
False.

True/False:
On the PowerEdge 2650, you must slide the riser board toward the expansion slot openings to remove the expansion-card riser board from the expansion-card cage.
False.
True.

True/False:
Memory banks must be populated sequentially on the PowerEdge 2650.
False.
True.

Multiple Choice:
On the PowerEdge 2650, where is the ROMB battery located?
Below the system fans.
Next to the memory.
Below the system board.
On the chassis wall.

True/False:
On the PowerEdge 2650, pin 1 on the processor must be aligned with pin 1 on the socket to properly replace the processor.
False.
True.

Choose all that apply:
On the PowerEdge 2650, what must be removed prior to removing a VRM?
Front bezel.
System cover.
Fan shroud.
System board.

True/False:
On the PowerEdge 2650, you must remove the four plastic retaining clips to remove the system board.
True.
False.

Multiple Choice:
What is the maximum number of PCI cards that can be installed in the PowerEdge 2650?
Four.
Five.
Three.
Two.

True/False:
The CD-ROM for the PowerEdge 2650 is SCSI.
True.
False.

True/False:
A single cable is required to connect the embedded SCSI controller to the SCSI backplane.
True.
False.

True/False:
The PowerEdge 2650 contains an integrated, Adaptec 7899, dual channel Ultra3 SCSI host adapter.
True.
False.

True/False:
The PowerEdge 2650 contains an integrated remote access card.
True.
False.

Multiple Choice:
What is the minimum number of power supplies required for the PowerEdge 2650?
One.
Two.
Six.
Four.

Multiple Choice:
How many DIMMs must be installed to utilize spare bank memory on the PowerEdge 2650?
Six.
Eight.
Four.
Two.

Multiple Choice:
How many DIMMs must be installed to utilize spare bank memory on the PowerEdge 2650?
Six.
Eight.
Four.
Two.

Multiple Choice:
What color latches on the slide rail assembly must you lift up to allow you to push the PowerEdge 2650 into a rack?
Brown.
Blue.
Yellow.
Green.

Multiple Choice:
Where is the system status indicator for the cable management arm plugged into on the PowerEdge 2650?
Below the power supplies.
Below the expansion-card cage.
Behind the front bezel.
Below the system identification indicator.

Multiple Choice:
What system setup option on the PowerEdge 2650 allows you to enable hyper-threading?
Boot sequence.
Integrated devices.
CPU information.
PCI IRQ assignment.

Multiple Choice:
What system setup option on the PowerEdge 2650 allows you to set the maximum memory available to the operating system to 256 MB?
Integrated devices.
PCI IRQ assignment.
OS install mode.
Embedded server management.

Multiple Choice:
If the ROMB hardware is installed, what system setup option on the PowerEdge 2650 allows you to enable or disable the embedded RAID controller?
Boot sequence.
Integrated devices.
Keyboard numlock.
PCI IRQ assignment.