What is the proper procedure to follow if the customer has a PowerVault 530F in their SAN?

   Do not perform any upgrade procedures. Use standard escalation procedures. *
 Insert the PowerVault 530F Upgrade disk into the PowerVault 530F and reboot the SAN appliance. 
 Insert the PowerVault 530F Upgrade disk into the PowerVault 530F. Click Appliance Upgrade. When prompted, reboot the appliance. 
 Upgrade all components in the SAN other than the PowerVault 530F. 

How do you determine the version of StorageC that is installed?

   The version can not be determined. 
 The version is listed in the service name. 
 The version is returned by the storagec info command line. This needs to be run from the c:\program files\openmanage\storage consolidation path. *
 The version is returned by the storagec -version command line. This needs to be run from the c:\program files\openmanage\storage consolidation path. 

What services must be stopped before upgrading the Qlogic Configuration Utility?

   Only the Win32SL needs to be stopped. 
 Before installing Qlconfig the QLConfig NT Agent service and the Win32SL service must be stopped. *
 Only the QLCOnfig NT Agent service needs to be stopped. 
 No services need to be stopped. 

How do you determine the version of QLDirect that is installed?

   The QLDirect version can not be determined. 
 Launch QLDirect, select about from the help menu. 
 The version is listed on the version tab in the qldirect.sys file properties. *
 Begin the upgrade procedure for QLDirect. If the installed version is the same or newer then the installer will advise and quit. If the installed version is older then the installer will proceed. 

Which of the following best describes the function of the QLogic Fibre Channel Configuration Utility (QLconfig)?

   Allows the OS to use and control the QLogic Fibre Channel HBA.  
 Provides data path failover for a server connected to a Dell PowerVault 65xF disk enclosure in a redundant configuration.  
 Establishes and manages data paths between servers and devices in the Fibre Channel SAN. *
 Serves as an SNMP proxy to help allow a server to configure and manage a Dell PowerVault 65xF disk enclosure. 

Which of the following best describes the function of Dell OpenManage Data Management Station (Data Supervisor)?

   Provides data path failover for a server connected to a Dell PowerVault 65xF disk enclosure in a redundant configuration. 
 Protects data by providing LUN masking for Microsoft Windows NT and Microsoft Windows 2000 operating systems. 
 Serves as an SNMP proxy to help allow a server to configure and manage a Dell PowerVault 65xF disk enclosure.  
 Provides a GUI management interface that is used to configure and manage a Dell PowerVault 65xF disk enclosure.* 

Which of the following best describes the function of Dell OpenManage Application Transparent Failover (ATF)?

   Establishes and manages data paths between servers and devices in the Fibre Channel SAN. 
 Provides data path failover for a server connected to a Dell PowerVault 65xF disk enclosure in a redundant configuration.  *
 Protects data by providing LUN masking for Microsoft Windows NT and Microsoft Windows 2000 operating systems. 
 Provides a GUI management interface that is used to configure and manage a Dell PowerVault 65xF disk enclosure. 

Which of the following best describes the function of Dell OpenManage Data Managed Node (Data Agent)?

   Provides a GUI management interface that is used to configure and manage a Dell PowerVault 65xF disk enclosure. 
 Provides data path failover for a server connected to a Dell PowerVault 65xF disk enclosure in a redundant configuration. 
 Establishes and manages data paths between servers and devices in the Fibre Channel SAN. 
 Serves as an SNMP proxy to help allow a server to configure and manage a Dell PowerVault 65xF disk enclosure. *

After flashing the RAID controllers in a PowerVault 660F and rebooting the enclosures Array Manager reports that the firmware hasn’t changed. What is the most likely cause?

   The server needs to be rebooted. 
 The switches need to be rebooted. 
 After the RAID controller firmware upgrade procedure the switch must be rezoned and the new paths set using QLconfig. If this is not done Array manager will only report cached information. *
 The enclosure needs to be rebooted. 

After flashing the RAID controllers Array manager reports that the enclosure did not respond to the reboot command. What is the most likely cause?

   The flash has failed. Reflash the enclosure. 
 This is normal. The proper procedure is to power cycle the enclosure. *
 This indicates a timeout condition. Click <Cancel>, perform a refresh and issue another reboot command. 
 This indicates that disks 0 through 3 have gone offline. Click , perform a re-scan, and issue another reboot command. 

What is the difference between part number 1G987 and part number 8K166?

   Part number 1G987 is a PowerVault 660F RAID controller that ships with 7.70 firmware. *
Part number 8K166 is a PowerVault 660F RAID controller that ships with 7.51 firmware. 
 1G987 is a PowerVault 660F RAID controller that ships without a firmware flash diskette. 
8K166 is a PowerVault 660F RAID controller that ships with a firmware flash diskette. 
 There is no difference. 
 Part number 1G987 is a PowerVault 660F RAID controller that ships with 7.51 firmware. 
Part number 8K166 is a PowerVault 660F RAID controller that ships with 7.70 firmware. 

On the PowerVault 660F, how does the World Wide Name propagation differ between the 7.51 RAID controller firmware and the 7.70 RAID controller firmware?

   The WWN propogates the same way in both firmware versions. *
 In the 7.70 firmware the WWN propagates from the primary controller to the secondary controller. In the 7.51 firmware the WWN propagates from the backplane to both controllers. 
 In the 7.51 firmware the WWN propagates from the secondary controller to the primary controller. In the 7.70 firmware the WWN propagates from the backplane to both controllers. 
 In the 7.51 firmware the WWN propagates from the primary controller to the secondary controller. In the 7.70 firmware the WWN propagates from the backplane to both controllers. 

Which of the following is the most likely cause for not being able to see the graphical screens in the Dell Switch Manager?

   The FC-AL address for the switch has been set incorrectly. 
 The system being used to access the switch does not have the Sun JavaSoft Java 1.2.2 browser plug-in installed. *
 The system accessing the switch is not a member of any Zone on the switch. 
 Dell Switch Manager has not been installed. 

Which of the following is the most likely to cause a DEFAULT STORAGE GROUP to appear in the Storage C Administrator?

   Data paths have not been configured between some of the servers and storage devices. *
 No servers have been configured as the MASTER from Storage C Administrator. 
 All of the servers and storage devices in the SAN are configured with factory defaults. 
 Dell OpenManage Storage Consolidation has not been installed on one or more servers in the SAN. 

Which of the following best describes the function of QLDirect?

   Provides data path failover for a server connected to a Dell PowerVault 660F storage system in a redundant configuration. *
 Allows the OS to use and control the QLogic Fibre Channel HBA. 
 Establishes and manages data paths between servers and devices in the Fibre Channel SAN. 
 Provides a GUI management interface that is used to configure and manage a Dell PowerVault 660F disk enclosure. 

Which of the following is used to configure virtual disks and perform management operations on the Dell PowerVault 660F?

   Dell OpenManage Data Managed Node. 
 Dell OpenManage Storage Consolidation. 
 Dell OpenManage Array Manager version 2.7.1 or later. *
 Dell OpenManage Data Management Station. 

 Which of the following Dell SAN 3.0 software components requires a CUSTOM installation to avoid errors associated with HP OpenView?

   Dell OpenManage Data Management Station (Data Supervisor). *
 Dell OpenManage Storage Consolidation (Storage C). 
 Dell OpenManage Data Managed Node (Data Agent). 
 Dell OpenManage Application Transparent Failover (ATF). 

What is the installation procedure for the Dell Switch Manager?

   Select Dell Switch Manager from the main menu on the SAN 3.0 Fibre Channel Update CD. 
 The Dell Switch Manager is installed as a component of the QLogic Fibre Channel Configuration Utility. 
 There is no installation procedure. The Dell Switch Manager is a feature of the switch firmware (Fabric OS). *
 The Dell Switch Manager is installed as a component of Dell OpenManage Data Management Station. 

Which of the following is an end point in the simplified Fibre Channel data flow model?

   A LUN on a Dell PowerVault DPE. *
 The QLogic HBA(s) in a server. 
 Fibre Channel switch. 
 Physical Media or Cabling. 


95%

Which of these should be configured prior to installing Dell OpenManage Storage Consolidation (Storage C)?
I. - Common Domain Membership.
II. - TCP/IP name resolution (hosts file or DNS).

   Neither I nor II. 
 I only. 
 II only. 
 Both I and II. *

What new feature does Qlconfig version 1.36+ provide?

   The new Qlogic Configuration Utility (1.36) adds support for dynamic re-pathing. 
 The new Qlogic Configuration Utility (1.36) adds support for setting a path to a private loop device. 
 No new features are added. 
 The new Qlogic Configuration Utility (1.36) adds support for the DMI subsystem in Windows 2000 Service Pack 2. *

What is the proper procedure to follow if you are replacing a RAID controller in a PowerVault 660F and the firmware revision on the replacement controller is different than the working controller?

   Do not replace the RAID controller. Call technical support. 
 Determine what firmware revision the surviving RAID controller is and flash the replacement controller to match. *
 Downgrade and replace as appropriate. 
 Upgrade and replace as appropriate. 

