Servers - PowerEdge 6400 Product Certification (37 Questions)

Multiple choice:
The PowerEdge 6400 has ___ 32-bit and __ 64-bit PCI expansion card slots.
Four, no
one, six
Three,no
one, three

True/False:
The PowerEdge 6400 supports 64-bit PCI expansion card slots.
FALSE.
TRUE.

Mutliple choice:
Which of the following type of RAM is used in the PowerEdge 6400?
ECC
DIMM
SDRAM
RIMM

True/False:
On the PowerEdge 6400, system memory DIMM modules must be installed in pairs.
False.
True.

Choose all that apply:
The following expansion card(s) are hot-pluggable on the PowerEdge 6400:
DRAC 2
QLogic HBA
ATI Rage Pro Video.
Intel Pro/100+ NIC.

Choose all that apply:
On the PowerEdge 6400, which of the following components are located on the system board?
Server Management Port
Adaptec 7899 SCSI controller
Intel Pro/100+ NIC
Audio

True/False:
The PowerEdge 6400 supports embedded RAID.
True.
False.

Multiple Choice:
Three SCSI backplanes available for the PowerEdge 6400 are:
1 x 3 and 1 x 6.
1 x 8, 1 x 6, and 2 x 3.
1 x 2, 1 x 6, and 1 x 8.
1 x 4 and 2 x 3.

Multiple choice:
The maximum number of hard-disk drives that can be installed in a PowerEdge 6400 is:
Ten.
Four.
Six.
Eight.

Multiple Choice:
The SCSI backplane on the PowerEdge 6400 is divided into a 2 X 4 split backplane by:
Installing a new split backplane.
Changing the system BIOS.
Installing an additional hard-disk drive.
Attaching a second SCSI cable.

Multiple choice:
On the PowerEdge 6400, prior to replacing the power supply, what must be done to the PowerEdge 6400, to ensure the procedure is completed safely?
Ground yourself to the PowerEdge 6400 only.
Unplug the AC power cable only.
Nothing, the power supply is hot-pluggable.
Power down and unplug the AC power.

Multiple choice:
On the PowerEdge 6400, when replacing the power supply, which of the following procedures should be performed to determine that the new power supply is functioning properly?
Run Dell diagnostics.
Power on the PowerEdge 6400 and watch for the green LED to light.
Power on the PowerEdge 6400 and access the event monitor to check that no events have occurred.
Power on the PowerEdge 6400 and wait for the POST to complete successfully.

True/False:
The hard drives on the PowerEdge 6400 are hot swappable.
True.
False.

Multiple choice:
On the PowerEdge 6400, prior to replacing one of the eight accessable hard drives, what must be done to the PowerEdge 6400, to ensure the procedure is completed safely?
Nothing, the hard-disk drive is hot-pluggable.
Power down and unplug the AC power.
Unplug the AC power cable only.
Ground yourself to the PowerEdge 6400 only.

Multiple choice:
On the PowerEdge 6400, prior to replacing a processor, what must be done to the PowerEdge 6400, to ensure the procedure is completed safely?
Unplug the AC power cable only.
Nothing, the processor is hot-pluggable.
Ground yourself to the PowerEdge 6400 only.
Power down and unplug the AC power.

Multiple Choice:
On the PowerEdge 6400, a 5/16 inch or a Torx 25 nut driver is used to remove the:
Power Supplies.
Processor Guides.
SCSI backplane.
CD-ROM drive bracket.

Choose all that apply:
To remove a system fan on the PowerEdge 6400, which one of the following tools are required:
Anti-static wrist strap.
3/16 inch nutdriver.
Your fingers.
#2 Phillips-head screwdriver.

True/False:
One of the two system fans on the PowerEdge 6400 is hot swappable one at a time.
True.
False.

Multiple choice:
Prior to replacing a system board, what must be done to the PowerEdge 6400 to ensure the procedure is completed safely?
Ground yourself to the PowerEdge 6400 only.
Unplug the AC power cable only.
Power down and unplug the AC power.
Nothing, the system board is hot-pluggable.

Multiple choice:
To remove the system board on the PowerEdge 6400, which one of the following components must first be removed:
The hard-disk drive fan pack.
The front bezel.
The power cabling harness.
The hard drive fan assembly.

True/False:
Following replacement of a system board due to failure, you should flash the BIOS on the new PowerEdge 6400 board to ensure the latest revision.
True.
False.

Multiple choice:
On the PowerEdge 6400, when replacing a SCSI backplane, which of the following procedures should be performed to determine that the new SCSI backplane is functioning properly?
Power on the PowerEdge 6400 and watch for the green LED to light.
Power on the PowerEdge 6400 and wait for the POST to complete successfully.
Run Dell diagnostics.
Power on the PowerEdge 6400 and access the event monitor to check that no events have occurred.

Choose all that apply:
To remove a SCSI backplane on the PowerEdge 6400, which of the following components must first be removed:
The PWR2 cable.
The right side cover.
The hard-disk drives.
The front bezel.

True/False:
When removing the PSPB on the PowerEdge 6400, slide it toward the power supplies after loosening the captive screw.
True.
False.

True/False:
On the PowerEdge 6400, install the highest-capacity DIMMS in Bank A first and the remaininng DIMMs in order of descending capacity in the remainng memory slots.
True.
False.

Choose all that apply:
The internal SCSI-3 twisted pair data cable can be connected between the:
SCSI backplane and Adaptec 7899 controller.
Hard-disk drive fan assembly and the SCSI backplane.
PSPB and SCSI bacckplane.
SCSI backplane and a PERC card.

Multiple choice:
On the PowerEdge 6400, the PCI expansion cards are secured to the chassis with:
A plastic hinged latch.
A metal hinged retainer.
One screw.
A black roller clip.

Multiple choice:
On the PowerEdge 6400, the PCI card insulation shroud is removed by pressing:
The retaining clip.
Two plastic clips.
The spring loaded screw.
The securing lever.

Multiple choice:
Remove the processor retention brackets on the PowerEdge 6400 using a:
Flat blade screw driver.
3/16 inch nut driver.
T-25 Torx nut driver.
Cresent wrench.