Servers - PowerEdge 1500SC Product Certification (15 Questions)

Multiple choice:
What type of RAM is used in the PowerEdge 1500SC?
DDR.
RAMBUS.
EDO.
SDRAM.

Multiple choice:
The PowerEdge 1500SC has ___ 32-bit and __ 64-bit PCI expansion card slots.
Two, Four
Four, Two
One, Four
Six, No

Choose all that apply:
On the PowerEdge 1500SC, which of the following components could be located on the system board?
SCSI controller.
Video.
Modem.
NIC.

True/False:
The PowerEdge 1500SC supports 64-bit PCI expansion card slots.
True.
False.

True/False:
The DIMMs in the PowerEdge 1500SC must be installed in pairs.
False.
True.

Multiple choice:
To remove the hard drives on the PowerEdge 1500SC, which one of the following components must be removed:
The hard drive fan assembly.
The power cabling harness.
The left side panel.
The front bezel.

True/False:
The redundant power supplies on the PowerEdge 1500SC are hot swappable.
True.
False.

Multiple Choice:
To remove the system memory on the PowerEdge 1500SC, which one of the following components must be removed.
The SCSI backplane.
The top cover.
The system board.
The right side panel.

Multiple Choice:
To remove the PSDB on the PowerEdge 1500SC, which one of the following components must first be removed.
The system board.
The top cover.
All installed PCI cards.
The system board.

Multiple choice:
To remove the SCSI backplane on the PowerEdge 1500SC, which one of the following components must first be removed:
The left side panel.
The hard-disk drives.
All installed PCI cards.
The system board.

Choose all that apply:
To remove the system fan on the PowerEdge 1500SC, which of the following components must be removed:
The top cover.
The right side panel.
The SCSI backplane.
The system board.

Multiple Choice:
To remove the system fan on the PowerEdge 1500SC, which one of the following components must be removed.
The power supplies.
The top cover.
The left side panel.
The right side panel.

Choose all that apply:
To remove the system fan on the PowerEdge 1500SC, which of the following components must first removed:
The CPU shroud.
The front bezel.
The left side panel.
All installed PCI cards.

Choose all that apply:
To remove standard non-redundant power supply the PowerEdge 1500SC, which one of the following components must be removed:
Nothing is needed to be removed first.
The left side panel.
The hard drive fan assembly.
The front bezel.

True/False:
On the PowerEdge 1500SC, processor slots that are not filled by a processor are required to be filled with a terminator card.
False.
True.