Choose All That Apply:
Which of the following devices must be removed prior to removing the Hard Drive Hood on the PowerEdge C1100? 

   Expander Board  
 Any attached peripherals  
= Cover  
 Hard Drives  

Which of the following cables must be disconnected prior to removing the Expander Board from the PowerEdge C1100? 

=   Power Cable  
= Fan cables  
= I2C communication cable  
 Midplane cable  

The PowerEdge C1100 supports memory mirroring. 

   TRUE 
= FALSE 

All PowerEdge C1100 systems come equipped with BMC including KVM and a dedicated NIC for the BMC. 

=   TRUE 
 FALSE 

What is the maximum amount of hard drives possible on the PowerEdge C1100? 

   24 
 12 
= 10 
 8 

Which of the following devices must be removed prior to removing the System Board on the PowerEdge C1100? 

=   Memory Modules  
 Heat Sink/Processor  
 Expansion Card Riser  
 Hard disk Drives  

How many total cables must be disconnected from the system board when removing the non-redundant power supply on the PowerEdge C1100? 

   1 
= 4 
 2 
 6 

Which of the following devices does NOT need to be removed prior to removing the System Board for the PowerEdge C1100? 

=   Hard Drive Hood  
 Memory Modules  
 Heat Sink/Processor  
 Expansion Card Riser  

How many PCIe slots are available in the PowerEdge C1100? 

=   One PCIe x16  
 Two PCIe x16  
 Two PCIe x8  
 One PCIe x8  


What is the maximum memory configuration available on the PowerEdge C1100? 

   64GB 
 72GB 
 96GB 
= 144GB 

The system Service Tag for the PowerEdge C1100 is located on the Main screen of the BIOS. 

=   FALSE 
 TRUE 

Which device must be removed immediately prior to removing the non-redundant power supply on the PowerEdge C1100? 

=   None, there are no prior device removals necessary.  
 Cooling Shroud  
 Expansion Board cable  
 Cover  


On the PowerEdge C1100, the BMC dedicated NIC is soldered to the system board. 

 ==  TRUE 
 FALSE 


On which screen of the BMC the PowerEdge C1100 would you find the Launch VM button to start a Virtual Media session? 

   Sensors tab  
 Configuration tab  
 == Console tab  
 System tab  




